(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Baby Mobile v5 — Key-Shaped Panel")
		(date "2026-03-11")
		(rev "5.0")
		(comment 1 "Carrier head + breakaway adapter stem")
		(comment 2 "Unique nets per sub-board, FPC interconnect")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0.05)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "/GND")
	(net 2 "/C_VBAT")
	(net 3 "/C_3V3")
	(net 4 "/AUDIO_OUT")
	(net 5 "/C_BTN3")
	(net 6 "/C_BTN1")
	(net 7 "unconnected-(FPC1-Pad13)")
	(net 8 "unconnected-(FPC1-Pad7)")
	(net 9 "unconnected-(FPC1-Pad14)")
	(net 10 "unconnected-(FPC1-Pad11)")
	(net 11 "/C_BTN4")
	(net 12 "unconnected-(FPC1-Pad15)")
	(net 13 "unconnected-(FPC1-Pad5)")
	(net 14 "unconnected-(FPC1-Pad6)")
	(net 15 "unconnected-(FPC1-Pad18)")
	(net 16 "/C_BTN2")
	(net 17 "unconnected-(FPC1-Pad12)")
	(net 18 "unconnected-(FPC1-Pad17)")
	(net 19 "/BOOST_SW")
	(net 20 "/AUDIO_PWM")
	(net 21 "/FLASH_CS")
	(net 22 "unconnected-(U1-FB-Pad2)")
	(net 23 "/SPI_MOSI")
	(net 24 "/SPI_SCK")
	(net 25 "/SPI_MISO")
	(net 26 "unconnected-(U3-VBUS-Pad14)")
	(net 27 "unconnected-(U3-P1.11_D6_TX-Pad7)")
	(net 28 "unconnected-(U3-P1.12_D7_RX-Pad8)")
	(net 29 "/A_GND")
	(net 30 "Net-(J1-Pin_15)")
	(net 31 "Net-(J1-Pin_4)")
	(net 32 "Net-(J1-Pin_7)")
	(net 33 "Net-(J1-Pin_12)")
	(net 34 "Net-(J1-Pin_11)")
	(net 35 "Net-(J1-Pin_5)")
	(net 36 "Net-(J1-Pin_13)")
	(net 37 "Net-(J1-Pin_10)")
	(net 38 "Net-(J1-Pin_3)")
	(net 39 "Net-(J1-Pin_6)")
	(net 40 "Net-(J1-Pin_8)")
	(net 41 "Net-(J1-Pin_16)")
	(net 42 "Net-(J1-Pin_9)")
	(net 43 "Net-(J1-Pin_14)")
	(net 44 "Net-(J1-Pin_1)")
	(net 45 "Net-(J1-Pin_2)")
	(net 46 "Net-(J2-Pin_7)")
	(net 47 "Net-(J2-Pin_6)")
	(net 48 "Net-(J2-Pin_15)")
	(net 49 "Net-(J2-Pin_1)")
	(net 50 "Net-(J2-Pin_5)")
	(net 51 "Net-(J2-Pin_8)")
	(net 52 "Net-(J2-Pin_10)")
	(net 53 "Net-(J2-Pin_2)")
	(net 54 "Net-(J2-Pin_13)")
	(net 55 "Net-(J2-Pin_14)")
	(net 56 "Net-(J2-Pin_9)")
	(net 57 "Net-(J2-Pin_16)")
	(net 58 "Net-(J2-Pin_12)")
	(net 59 "Net-(J2-Pin_3)")
	(net 60 "Net-(J2-Pin_4)")
	(net 61 "Net-(J2-Pin_11)")
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(uuid "0697cdb8-fbfb-41c5-9cbe-5465e1ced395")
		(at 123.75 112.0875 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 -1.55 90)
			(layer "F.SilkS")
			(uuid "7889443f-1360-4bc3-b8f1-94d704c08b2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7uH"
			(at 0 1.55 90)
			(layer "F.Fab")
			(uuid "fbd97374-ac02-4dce-8dd4-6c201be8be29")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "2ff0360f-cdcd-47a6-876e-904043e8df9b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "29fdc5fb-f475-4138-a0c0-b4a7ae88b06c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/c358b595-8b13-497e-9e9e-49f65d43ca20")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.399622 -0.56)
			(end 0.399622 -0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77f72ebe-41e1-4d6d-87f3-92f502e04086")
		)
		(fp_line
			(start -0.399622 0.56)
			(end 0.399622 0.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7011afcc-176c-45f2-a608-ed7cfc805d7c")
		)
		(fp_line
			(start 1.75 -0.85)
			(end 1.75 0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f51fd6b-1896-41ff-9d44-302d73b71c0c")
		)
		(fp_line
			(start -1.75 -0.85)
			(end 1.75 -0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c71dcac7-9dba-4c30-8cc6-decc23c0aa77")
		)
		(fp_line
			(start 1.75 0.85)
			(end -1.75 0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "065a64ef-ca9f-4d57-8ea8-5a6f3c218e92")
		)
		(fp_line
			(start -1.75 0.85)
			(end -1.75 -0.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24fcdb59-5d1b-44ec-9c64-4593cce57488")
		)
		(fp_line
			(start 1 -0.45)
			(end 1 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19497772-1755-4b51-97cc-fd8e1ff67db1")
		)
		(fp_line
			(start -1 -0.45)
			(end 1 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd466f2a-a2a2-4542-be78-7e260000f9d4")
		)
		(fp_line
			(start 1 0.45)
			(end -1 0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7acbf891-f8e9-4771-ba6e-6763505ff3ba")
		)
		(fp_line
			(start -1 0.45)
			(end -1 -0.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14653a13-b51c-4c45-94ad-c7aa149b2acb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c088d7f0-4809-4a64-8b89-0dc14fe69123")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/C_VBAT")
			(pinfunction "1")
			(pintype "passive")
			(uuid "d9151b83-f4dc-430e-962f-827d7464229a")
		)
		(pad "2" smd roundrect
			(at 1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/BOOST_SW")
			(pinfunction "2")
			(pintype "passive")
			(uuid "abe7efdf-4efe-441d-b524-35c175dd70b4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EasyEDA_Lib:FPC-SMD_16P-P0.50_FPC16-T1T1-2020-A"
		(layer "F.Cu")
		(uuid "1ec63236-3944-4d63-a359-2a6c288b31ec")
		(at 107.44 124.7125)
		(property "Reference" "FPC1"
			(at 0 -2.6125 0)
			(layer "F.SilkS")
			(uuid "29c1a3c1-5579-480d-ad9b-1dd4b501d229")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "FPC-20 Carrier"
			(at 0 5.057 0)
			(layer "F.Fab")
			(uuid "1a09455f-e355-46c1-b1c2-af8a0f185187")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://item.szlcsc.com/datasheet/FPC16-T1T1-2020-A/55627462.html"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0559770-d3ff-4a1c-b5b8-6b81c86632f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Locking Feature:Hinged Lid Contact Type:Bottom Contact Number of Contacts:16P Pitch:0.5mm Mounting Type:Surface Mount, Right Angle FFC, FCB Thickness:0.3mm FFC, FCB Thickness:0.3mm Height Above Board:2mm Contact Material:Copper Contact Plating:Tin Rated V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef83f6ec-c7ca-4244-8bfc-6b28e1b6631f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "JLC_3DModel_Q" "7d16379a8679465dac6cebcc2a0d3734"
			(at 0 0 0)
			(layer "Cmts.User")
			(hide yes)
			(uuid "29f49d57-4744-467e-a741-cbee3666d369")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "JLC_3D_Size" "12.41 5.87"
			(at 0 0 0)
			(layer "Cmts.User")
			(hide yes)
			(uuid "9a85f331-89c5-4d1e-b34a-a92659bcf8a4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer Part" "FPC16-T1T1-2020-A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "396a1e7a-528a-45cc-95cb-db7aaf491814")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "SHETIME(高钺达)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fda1af36-99d9-4e84-a661-c80811418008")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part" "C52740846"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "878c632e-7b4d-4a6e-9d00-835f1320e87e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier" "LCSC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7dbe0bdc-e9f7-4bfb-8cb4-7abe3b5c64a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC Part Name" "翻盖式 下接 P数:16P 间距:0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4cc3c413-3174-4239-a5e6-465a810d0f91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/9426180e-9cc5-457d-9538-1387435d67fd")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(fp_line
			(start -6.25 -0.762)
			(end -4.131 -0.762)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "09fdedcd-090a-4265-9f4d-ff32bce310f3")
		)
		(fp_line
			(start -6.25 -0.1935)
			(end -6.25 -0.762)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "ed409c87-1338-4d8c-87e2-136981f24140")
		)
		(fp_line
			(start -6.25 4.23)
			(end -6.25 2.7685)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "862fab89-77e2-4656-ba64-f9f3d01c8fc8")
		)
		(fp_line
			(start -6.25 4.23)
			(end 6.25 4.23)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "31e2e799-a388-4f73-87bd-df492f44fbda")
		)
		(fp_line
			(start 6.25 -0.762)
			(end 4.131 -0.762)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "62def645-96d3-402c-8be1-a22c52cdf5dc")
		)
		(fp_line
			(start 6.25 -0.1935)
			(end 6.25 -0.762)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "99c6edf1-e082-4e59-8617-6fd3ee975e80")
		)
		(fp_line
			(start 6.25 4.23)
			(end 6.25 2.7685)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "eb1f6e05-dd24-4c1c-9afd-4dc30e8893c8")
		)
		(fp_poly
			(pts
				(arc
					(start -4.992 -1.397)
					(mid -4.581 -1.808)
					(end -4.17 -1.397)
				)
				(arc
					(start -4.17 -1.397)
					(mid -4.581 -0.986)
					(end -4.992 -1.397)
				)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "9bc193d1-9702-412d-b854-741e8bae9f72")
		)
		(fp_poly
			(pts
				(arc
					(start -6.073 4.2)
					(mid -6.2 4.327)
					(end -6.327 4.2)
				)
				(arc
					(start -6.327 -0.7)
					(mid -6.2 -0.827)
					(end -6.073 -0.7)
				)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "b4574a08-ea5e-40c2-be64-a106556c9e3a")
		)
		(fp_poly
			(pts
				(arc
					(start -6.2 -0.573)
					(mid -6.327 -0.7)
					(end -6.2 -0.827)
				)
				(arc
					(start 6.2 -0.827)
					(mid 6.289803 -0.789803)
					(end 6.327 -0.7)
				)
				(arc
					(start 6.327 4.2)
					(mid 6.289803 4.289803)
					(end 6.2 4.327)
				)
				(arc
					(start -6.2 4.327)
					(mid -6.327 4.2)
					(end -6.2 4.073)
				)
				(xy 6.073 4.073) (xy 6.073 -0.573)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "68e36d6b-5cb0-44ba-8b2c-700160047744")
		)
		(fp_poly
			(pts
				(xy -6.19 0.5375) (xy -4.69 0.5375) (xy -4.69 2.0375) (xy -6.19 2.0375)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "a0b7d634-2e7d-4efc-8392-88c68419072f")
		)
		(fp_poly
			(pts
				(xy -3.9 -1.5125) (xy -3.6 -1.5125) (xy -3.6 -0.6625) (xy -3.9 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "0544e224-7635-470c-968b-7c67f22e1e79")
		)
		(fp_poly
			(pts
				(xy -3.4 -1.5125) (xy -3.1 -1.5125) (xy -3.1 -0.6625) (xy -3.4 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "8123c216-01f7-4174-bb80-6aacb99de49b")
		)
		(fp_poly
			(pts
				(xy -2.9 -1.5125) (xy -2.6 -1.5125) (xy -2.6 -0.6625) (xy -2.9 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "959aa0d1-208d-44ee-96fc-849ed566f663")
		)
		(fp_poly
			(pts
				(xy -2.4 -1.5125) (xy -2.1 -1.5125) (xy -2.1 -0.6625) (xy -2.4 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "83ec6c13-79ba-4acb-9741-961def2e70cd")
		)
		(fp_poly
			(pts
				(xy -1.9 -1.5125) (xy -1.6 -1.5125) (xy -1.6 -0.6625) (xy -1.9 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "473fd1ba-fb7c-4d06-9f3d-1b84d7c40dc8")
		)
		(fp_poly
			(pts
				(xy -1.4 -1.5125) (xy -1.1 -1.5125) (xy -1.1 -0.6625) (xy -1.4 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "d06dc383-67d1-4d80-b696-913074add1db")
		)
		(fp_poly
			(pts
				(xy -0.9 -1.5125) (xy -0.6 -1.5125) (xy -0.6 -0.6625) (xy -0.9 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "3a2d901f-d944-44e5-a564-b44beb281581")
		)
		(fp_poly
			(pts
				(xy -0.4 -1.5125) (xy -0.1 -1.5125) (xy -0.1 -0.6625) (xy -0.4 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "52c9c1f4-e37b-4274-ad10-18c8cc4fa113")
		)
		(fp_poly
			(pts
				(xy 0.1 -1.5125) (xy 0.4 -1.5125) (xy 0.4 -0.6625) (xy 0.1 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "1a27a034-285a-4751-90d3-ae566b84186c")
		)
		(fp_poly
			(pts
				(xy 0.6 -1.5125) (xy 0.9 -1.5125) (xy 0.9 -0.6625) (xy 0.6 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "c7017d1b-b13a-477f-a198-d1b63a80843c")
		)
		(fp_poly
			(pts
				(xy 1.1 -1.5125) (xy 1.4 -1.5125) (xy 1.4 -0.6625) (xy 1.1 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "d6ca3d72-6142-4c77-81d5-5a24a6c897d3")
		)
		(fp_poly
			(pts
				(xy 1.6 -1.5125) (xy 1.9 -1.5125) (xy 1.9 -0.6625) (xy 1.6 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "5baf8ea2-c448-4b63-9fc9-812fc6d0907b")
		)
		(fp_poly
			(pts
				(xy 2.1 -1.5125) (xy 2.4 -1.5125) (xy 2.4 -0.6625) (xy 2.1 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "2724a9a4-7d30-4564-947f-812245bfa359")
		)
		(fp_poly
			(pts
				(xy 2.6 -1.5125) (xy 2.9 -1.5125) (xy 2.9 -0.6625) (xy 2.6 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "af0c1928-407f-4910-a590-dfd80048b9e3")
		)
		(fp_poly
			(pts
				(xy 3.1 -1.5125) (xy 3.4 -1.5125) (xy 3.4 -0.6625) (xy 3.1 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "5c2487a3-1a3b-4159-b6eb-99d84db83cce")
		)
		(fp_poly
			(pts
				(xy 3.6 -1.5125) (xy 3.9 -1.5125) (xy 3.9 -0.6625) (xy 3.6 -0.6625)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "e74b2f92-27f6-43c1-ba11-3eca17c618b9")
		)
		(fp_poly
			(pts
				(xy 4.69 0.5375) (xy 6.19 0.5375) (xy 6.19 2.0375) (xy 4.69 2.0375)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "11aec126-a690-4683-a4ec-48bd7c4af4ff")
		)
		(fp_line
			(start -6.2 -0.89)
			(end -6.2 4.23)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "faadca19-cce1-46a2-9ecf-05b938ad94c6")
		)
		(fp_line
			(start -6.2 4.23)
			(end 6.2 4.23)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "1ba93888-c8bd-4ae4-bc2d-4838672210bd")
		)
		(fp_line
			(start 6.2 -0.89)
			(end -6.2 -0.89)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "d46cd278-dbf7-437a-bcfd-8db771908e5f")
		)
		(fp_line
			(start 6.2 4.23)
			(end 6.2 -0.89)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "e99fb6a3-c7cf-473d-b39a-c1b338338832")
		)
		(fp_poly
			(pts
				(xy -6.144567 -1.535461) (xy -6.177039 -1.567933) (xy -6.222961 -1.567933) (xy -6.255433 -1.535461)
				(xy -6.255433 -1.489539) (xy -6.222961 -1.457067) (xy -6.177039 -1.457067) (xy -6.144567 -1.489539)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.3")
			(uuid "702783ce-565c-49ad-bd07-6b53b4c403cb")
		)
		(pad "1" smd rect
			(at -3.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/C_BTN1")
			(pinfunction "1")
			(pintype "unspecified")
			(uuid "1291469c-ab30-49c3-b981-600b95ae1709")
		)
		(pad "2" smd rect
			(at -3.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/C_BTN2")
			(pinfunction "2")
			(pintype "unspecified")
			(uuid "954292ff-6709-450e-af7f-b8dc1305a1a7")
		)
		(pad "3" smd rect
			(at -2.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/C_BTN3")
			(pinfunction "3")
			(pintype "unspecified")
			(uuid "0b2599ab-2b55-4075-8030-52bba8764dc1")
		)
		(pad "4" smd rect
			(at -2.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/C_BTN4")
			(pinfunction "4")
			(pintype "unspecified")
			(uuid "5929a05c-424e-4ba9-9e9d-9cdc7b43da31")
		)
		(pad "5" smd rect
			(at -1.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(FPC1-Pad5)")
			(pinfunction "5")
			(pintype "unspecified")
			(uuid "751100d8-9427-4645-afd1-8e12ade9bc56")
		)
		(pad "6" smd rect
			(at -1.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(FPC1-Pad6)")
			(pinfunction "6")
			(pintype "unspecified")
			(uuid "7bdff858-7ce1-491e-9092-7c30032eeab9")
		)
		(pad "7" smd rect
			(at -0.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(FPC1-Pad7)")
			(pinfunction "7")
			(pintype "unspecified")
			(uuid "3fde4e84-4ae9-441a-9725-ec595fbacca9")
		)
		(pad "8" smd rect
			(at -0.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/C_3V3")
			(pinfunction "8")
			(pintype "unspecified")
			(uuid "8a632182-5067-4dce-b767-c5cc8e337ad3")
		)
		(pad "9" smd rect
			(at 0.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/GND")
			(pinfunction "9")
			(pintype "unspecified")
			(uuid "5a1cf7a2-cca0-46b4-9d88-d7fffb60025e")
		)
		(pad "10" smd rect
			(at 0.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/C_VBAT")
			(pinfunction "10")
			(pintype "unspecified")
			(uuid "bf38b4ae-2616-4780-b42c-e0adf0e47bae")
		)
		(pad "11" smd rect
			(at 1.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(FPC1-Pad11)")
			(pinfunction "11")
			(pintype "unspecified")
			(uuid "4a12a722-aba4-49e5-a739-c987e3ddb9df")
		)
		(pad "12" smd rect
			(at 1.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(FPC1-Pad12)")
			(pinfunction "12")
			(pintype "unspecified")
			(uuid "b302c7f9-4b2d-4816-b0af-e6207672cccf")
		)
		(pad "13" smd rect
			(at 2.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(FPC1-Pad13)")
			(pinfunction "13")
			(pintype "unspecified")
			(uuid "17d37efd-b3ec-4035-bdc1-37ad259cc30f")
		)
		(pad "14" smd rect
			(at 2.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(FPC1-Pad14)")
			(pinfunction "14")
			(pintype "unspecified")
			(uuid "42605141-f98c-4799-8a89-a21b9b33d6d5")
		)
		(pad "15" smd rect
			(at 3.25 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(FPC1-Pad15)")
			(pinfunction "15")
			(pintype "unspecified")
			(uuid "5f4ba770-d930-47d2-98cf-49084cc65707")
		)
		(pad "16" smd rect
			(at 3.75 -1.2875)
			(size 0.3 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/AUDIO_OUT")
			(pinfunction "16")
			(pintype "unspecified")
			(uuid "4a74a4ad-a68a-4cb5-be9b-c12841ea5ec0")
		)
		(pad "17" smd rect
			(at 5.44 1.2875)
			(size 2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(FPC1-Pad17)")
			(pinfunction "17")
			(pintype "unspecified")
			(uuid "f8aaaeec-204d-4606-bd9b-a872305d28ab")
		)
		(pad "18" smd rect
			(at -5.44 1.2875)
			(size 2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(FPC1-Pad18)")
			(pinfunction "18")
			(pintype "unspecified")
			(uuid "871d26ac-acc6-48d9-99d2-cc718f063dd8")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/EASYEDA_MODELS/FPC-SMD_16P-P0.50_FPC16-T1T1-2020-A.step"
			(offset
				(xyz 0 -1.481 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "EasyEDA_Lib:FPC-SMD_HCTL_HC-FPC-03-10-17RLTAG"
		(layer "F.Cu")
		(uuid "2029c86c-50f2-4556-8c58-1cffda3335eb")
		(at 122.25 143.02775)
		(property "Reference" "FPC2"
			(at 0 -2.69 0)
			(layer "F.SilkS")
			(uuid "d1702399-5fea-4795-b815-4d741610d218")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "FPC-20 SOP-16N"
			(at 0 3.367 0)
			(layer "F.Fab")
			(uuid "22f94bec-e8f8-4d16-b65c-b50649d37888")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://item.szlcsc.com/datasheet/FPC16-T1T1-2020-A/55627462.html"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "53a7862a-6ade-4501-a436-555fa85d91f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Locking Feature:Hinged Lid Contact Type:Bottom Contact Number of Contacts:16P Pitch:0.5mm Mounting Type:Surface Mount, Right Angle FFC, FCB Thickness:0.3mm FFC, FCB Thickness:0.3mm Height Above Board:2mm Contact Material:Copper Contact Plating:Tin Rated V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5108cc7e-2db8-43e9-b402-396d8a899973")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer Part" "FPC16-T1T1-2020-A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "83a54d65-1d7e-4c3a-880e-f9f78dcdaf76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "SHETIME(高钺达)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d32c44f-aa5b-44ff-b7b6-64cd9b84e655")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part" "C52740846"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4fec57b-8b13-496d-83e4-bbc692205c7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier" "LCSC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d9f10abf-a875-402a-baf0-830596d8e193")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC Part Name" "翻盖式 下接 P数:16P 间距:0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "49f2ccbd-b395-43fe-9605-d8693c1562a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/1e20e107-cee6-42e8-a075-64e6e08c59d3")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(fp_line
			(start -3.3 -1.44)
			(end -3.3 0.247)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "d4d79fd3-133b-4bd9-bb38-20fb906e0053")
		)
		(fp_line
			(start -3.3 -1.44)
			(end -2.481 -1.44)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "a3590717-d818-4055-b900-22f0a5ed14b4")
		)
		(fp_line
			(start 2.4815 -1.44)
			(end 3.3 -1.44)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "23eb32c7-fe9b-413b-9310-ca2557e26601")
		)
		(fp_line
			(start 3.3 -1.44)
			(end 3.3 0.247)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "69471489-906b-4e9c-a083-6bbe4a13fba6")
		)
		(fp_circle
			(center -2.417 2.413)
			(end -2.29 2.413)
			(stroke
				(width 0.254)
				(type default)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "472acb1f-e145-40d6-b975-81405883c365")
		)
		(fp_poly
			(pts
				(xy -3.302 1.397) (xy -3.302 2.032) (xy -3.175 2.032) (xy -3.175 1.397)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "4dee160c-a36e-4f67-9f75-38c8431563a6")
		)
		(fp_poly
			(pts
				(xy 3.175 2.032) (xy -3.175 2.032) (xy -3.175 1.905) (xy 3.175 1.905)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "351b83a4-7f11-4e91-a544-88948134a8f7")
		)
		(fp_poly
			(pts
				(xy 3.302 1.397) (xy 3.302 2.032) (xy 3.175 2.032) (xy 3.175 1.397)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "d02008f0-b69b-42c6-bacd-39eb51e5c664")
		)
		(fp_poly
			(pts
				(xy -3.16 0.54) (xy -3.04 0.54) (xy -3.04 1.54) (xy -3.16 1.54)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "60bc6cfd-d36e-42be-b3f5-e8fe39385874")
		)
		(fp_poly
			(pts
				(xy -2.46 1.29) (xy -2.34 1.29) (xy -2.34 1.79) (xy -2.46 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "f948a6a6-5f68-4d48-911d-5dc7e1260319")
		)
		(fp_poly
			(pts
				(xy -2.1595 -1.69) (xy -2.0395 -1.69) (xy -2.0395 -1.19) (xy -2.1595 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "f818283e-36e8-4165-8b59-5dcc5539620a")
		)
		(fp_poly
			(pts
				(xy -1.8595 1.29) (xy -1.7395 1.29) (xy -1.7395 1.79) (xy -1.8595 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "d295f568-0f7b-4998-8ecc-30ebaf18e162")
		)
		(fp_poly
			(pts
				(xy -1.5595 -1.69) (xy -1.4395 -1.69) (xy -1.4395 -1.19) (xy -1.5595 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "03177db2-8b27-4239-bcdc-79b060fb8ca5")
		)
		(fp_poly
			(pts
				(xy -1.26 1.29) (xy -1.14 1.29) (xy -1.14 1.79) (xy -1.26 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "6de31a9f-ac3d-447d-beff-bf2c9447a4e1")
		)
		(fp_poly
			(pts
				(xy -0.96 -1.69) (xy -0.84 -1.69) (xy -0.84 -1.19) (xy -0.96 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "0b4933bb-edde-40ae-8fa0-40cd1724e82c")
		)
		(fp_poly
			(pts
				(xy -0.66 1.29) (xy -0.54 1.29) (xy -0.54 1.79) (xy -0.66 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "57460333-47bc-477b-81ae-65ca57f5b5b1")
		)
		(fp_poly
			(pts
				(xy -0.36 -1.69) (xy -0.24 -1.69) (xy -0.24 -1.19) (xy -0.36 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "d4b3e09f-0bcb-49ef-8a1a-b2529e4d6e7c")
		)
		(fp_poly
			(pts
				(xy -0.06 1.29) (xy 0.06 1.29) (xy 0.06 1.79) (xy -0.06 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "0d95ea5a-1034-4a1c-9fcd-eeec3579f4d1")
		)
		(fp_poly
			(pts
				(xy 0.24 -1.69) (xy 0.36 -1.69) (xy 0.36 -1.19) (xy 0.24 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "cd4e7793-9a61-4469-98ba-0b3704974a13")
		)
		(fp_poly
			(pts
				(xy 0.54 1.29) (xy 0.66 1.29) (xy 0.66 1.79) (xy 0.54 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "b00f74af-6308-487b-aefe-38a753efe428")
		)
		(fp_poly
			(pts
				(xy 0.8405 -1.69) (xy 0.9605 -1.69) (xy 0.9605 -1.19) (xy 0.8405 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "93e966a3-c6a5-420c-9a0b-6d0ec572ecb8")
		)
		(fp_poly
			(pts
				(xy 1.1405 1.29) (xy 1.2605 1.29) (xy 1.2605 1.79) (xy 1.1405 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "2ed5c6fc-ac79-43b7-874b-0cb334dc4521")
		)
		(fp_poly
			(pts
				(xy 1.4405 -1.69) (xy 1.56 -1.69) (xy 1.56 -1.19) (xy 1.4405 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "92b79457-4173-4faa-88e4-c6ce9f5f6178")
		)
		(fp_poly
			(pts
				(xy 1.74 1.29) (xy 1.86 1.29) (xy 1.86 1.79) (xy 1.74 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "a0593591-019d-4c2e-a56c-8d29beedb22e")
		)
		(fp_poly
			(pts
				(xy 2.04 -1.69) (xy 2.16 -1.69) (xy 2.16 -1.19) (xy 2.04 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "b82c776f-93e4-4d91-81bb-0c59cbb2105d")
		)
		(fp_poly
			(pts
				(xy 2.34 1.29) (xy 2.46 1.29) (xy 2.46 1.79) (xy 2.34 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "057fbe19-7c10-48e9-b499-043f6d6a4f80")
		)
		(fp_poly
			(pts
				(xy 3.04 0.54) (xy 3.16 0.54) (xy 3.16 1.54) (xy 3.04 1.54)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "b8ccd6ca-77d6-4319-8753-27de89664851")
		)
		(fp_line
			(start -3.3 -1.44)
			(end 3.3 -1.44)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "803ab0b5-b394-4e5f-a923-fa5d5332fc73")
		)
		(fp_line
			(start -3.3 1.96)
			(end -3.3 -1.44)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "8a7e1a86-a491-44e9-8770-557a9010be09")
		)
		(fp_line
			(start 3.3 -1.44)
			(end 3.3 1.96)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "da82362d-d61f-4651-904d-ba662d9b7c50")
		)
		(fp_line
			(start 3.3 1.96)
			(end -3.3 1.96)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "82018aa3-93d4-40be-8488-79998119a0e7")
		)
		(fp_poly
			(pts
				(xy -3.244567 1.937039) (xy -3.277039 1.904567) (xy -3.322961 1.904567) (xy -3.355433 1.937039)
				(xy -3.355433 1.982961) (xy -3.322961 2.015433) (xy -3.277039 2.015433) (xy -3.244567 1.982961)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.3")
			(uuid "549303de-4324-41d5-8d99-89f993ae2da4")
		)
		(pad "1" smd rect
			(at -2.4 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(J1-Pin_1)")
			(pinfunction "1")
			(pintype "unspecified")
			(uuid "d4336d4c-5aa2-42d9-8a03-a4874f579eda")
		)
		(pad "2" smd rect
			(at -2.0995 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "Net-(J1-Pin_2)")
			(pinfunction "2")
			(pintype "unspecified")
			(uuid "e0d31393-fae0-4983-9b07-2c9e66f7eb8f")
		)
		(pad "3" smd rect
			(at -1.7995 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "Net-(J1-Pin_3)")
			(pinfunction "3")
			(pintype "unspecified")
			(uuid "9dcebf33-31d1-4374-962f-84f65654e58a")
		)
		(pad "4" smd rect
			(at -1.4995 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(J1-Pin_4)")
			(pinfunction "4")
			(pintype "unspecified")
			(uuid "232f7af6-41b0-4623-a0c7-8418abcf5719")
		)
		(pad "5" smd rect
			(at -1.2 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(J1-Pin_5)")
			(pinfunction "5")
			(pintype "unspecified")
			(uuid "612ac576-82ee-4ad7-91ba-b9fddf23e3ec")
		)
		(pad "6" smd rect
			(at -0.9 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(J1-Pin_6)")
			(pinfunction "6")
			(pintype "unspecified")
			(uuid "9ee6b259-80aa-4720-875d-ed41d0499574")
		)
		(pad "7" smd rect
			(at -0.6 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "Net-(J1-Pin_7)")
			(pinfunction "7")
			(pintype "unspecified")
			(uuid "42af9114-a7a0-4bcc-ab64-4cc218b86bbd")
		)
		(pad "8" smd rect
			(at -0.3 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Net-(J1-Pin_8)")
			(pinfunction "8")
			(pintype "unspecified")
			(uuid "ae4c42b0-67c5-409a-9ee9-db1a4d63b58a")
		)
		(pad "9" smd rect
			(at 0 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(J1-Pin_9)")
			(pinfunction "9")
			(pintype "unspecified")
			(uuid "b21abac8-87db-4f9f-a257-d3f82f204438")
		)
		(pad "10" smd rect
			(at 0.3 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(J1-Pin_10)")
			(pinfunction "10")
			(pintype "unspecified")
			(uuid "8868b421-b7d1-45d8-bf0b-3e9431d704be")
		)
		(pad "11" smd rect
			(at 0.6 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(J1-Pin_11)")
			(pinfunction "11")
			(pintype "unspecified")
			(uuid "60d258a9-9077-4a04-9cae-9e7e4f6c06e8")
		)
		(pad "12" smd rect
			(at 0.9005 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(J1-Pin_12)")
			(pinfunction "12")
			(pintype "unspecified")
			(uuid "5a6835f3-66c0-4bc3-827a-07a2ea769a92")
		)
		(pad "13" smd rect
			(at 1.2005 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(J1-Pin_13)")
			(pinfunction "13")
			(pintype "unspecified")
			(uuid "860bae6f-73af-41d2-91ae-d5876b1e8eb3")
		)
		(pad "14" smd rect
			(at 1.5005 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(J1-Pin_14)")
			(pinfunction "14")
			(pintype "unspecified")
			(uuid "c113166e-cda2-4874-99b3-9848dcaa8b19")
		)
		(pad "15" smd rect
			(at 1.8 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(J1-Pin_15)")
			(pinfunction "15")
			(pintype "unspecified")
			(uuid "14d392ee-1ac7-4867-973e-2c3694611799")
		)
		(pad "16" smd rect
			(at 2.1 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "Net-(J1-Pin_16)")
			(pinfunction "16")
			(pintype "unspecified")
			(uuid "af246091-e7e7-4ace-b354-5a6de1b2fd8a")
		)
		(pad "17" smd rect
			(at 2.4 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/A_GND")
			(pinfunction "17")
			(pintype "unspecified")
			(uuid "c25efb24-b64a-43c8-8b8e-41c88aaaa70f")
		)
		(pad "18" smd rect
			(at 3.1 1.04)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/A_GND")
			(pinfunction "18")
			(pintype "unspecified")
			(uuid "a47bce9a-376d-4a4a-acfb-45485ab7d32a")
		)
		(pad "19" smd rect
			(at -3.1 1.04)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "2a80d6ad-fc76-4b7f-8fb2-629bf6f444ef")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/EASYEDA_MODELS/FPC-SMD_HCTL_HC-FPC-03-10-17RLTAG.step"
			(offset
				(xyz 0 -0.127 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "EasyEDA_Lib:FPC-SMD_HCTL_HC-FPC-03-10-17RLTAG"
		(layer "F.Cu")
		(uuid "2298bc7e-9a92-4d8e-a7e6-46397425c357")
		(at 103.5 143.0375)
		(property "Reference" "FPC3"
			(at 0 -2.69 0)
			(layer "F.SilkS")
			(uuid "a201a444-3484-490f-b866-81f38155919d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "FPC-20 SOP-16N"
			(at 0 3.367 0)
			(layer "F.Fab")
			(uuid "1a587fca-45ff-4019-b303-37bbfce6cd98")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://item.szlcsc.com/datasheet/FPC16-T1T1-2020-A/55627462.html"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "762b63c4-44d2-4d17-95d3-c77623607f0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Locking Feature:Hinged Lid Contact Type:Bottom Contact Number of Contacts:16P Pitch:0.5mm Mounting Type:Surface Mount, Right Angle FFC, FCB Thickness:0.3mm FFC, FCB Thickness:0.3mm Height Above Board:2mm Contact Material:Copper Contact Plating:Tin Rated V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "de4475a4-7d8d-4f49-ac83-03c74bb792f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer Part" "FPC16-T1T1-2020-A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "42f78eb0-d5f8-4d91-b867-21760a0ac0e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "SHETIME(高钺达)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "21660733-4615-4fb9-b87e-c1ff5361fd25")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part" "C52740846"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff931643-7e13-4e57-b523-c49841d727c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier" "LCSC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2970d308-409d-4c0e-bd86-8c72465b83a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC Part Name" "翻盖式 下接 P数:16P 间距:0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0de845d-263b-4406-9c8e-22bad0feee51")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/f5439f69-9c2f-4763-8702-073ccb6b46c9")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(fp_line
			(start -3.3 -1.44)
			(end -3.3 0.247)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "8ed57b16-851f-47ee-8fe2-e7ecc74627b8")
		)
		(fp_line
			(start -3.3 -1.44)
			(end -2.481 -1.44)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "fc07006a-4e14-4539-930e-e96c7ba606d7")
		)
		(fp_line
			(start 2.4815 -1.44)
			(end 3.3 -1.44)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "9cdb8be4-ab8c-4528-93c8-2c9415d7de43")
		)
		(fp_line
			(start 3.3 -1.44)
			(end 3.3 0.247)
			(stroke
				(width 0.254)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "20febfe6-44e6-4df6-9f37-c9108beb0193")
		)
		(fp_circle
			(center -2.417 2.413)
			(end -2.29 2.413)
			(stroke
				(width 0.254)
				(type default)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "f4a16463-7d21-4443-a85d-061b99223cfd")
		)
		(fp_poly
			(pts
				(xy -3.302 1.397) (xy -3.302 2.032) (xy -3.175 2.032) (xy -3.175 1.397)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "57cadffe-5e70-4dc7-8317-f253f263bdaf")
		)
		(fp_poly
			(pts
				(xy 3.175 2.032) (xy -3.175 2.032) (xy -3.175 1.905) (xy 3.175 1.905)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "d7939b85-3fd3-429c-969b-bf1bd20cb499")
		)
		(fp_poly
			(pts
				(xy 3.302 1.397) (xy 3.302 2.032) (xy 3.175 2.032) (xy 3.175 1.397)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "Dwgs.User")
			(uuid "6ddbe6c1-a5c3-495c-aea7-cf5ecf94275c")
		)
		(fp_poly
			(pts
				(xy -3.16 0.54) (xy -3.04 0.54) (xy -3.04 1.54) (xy -3.16 1.54)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "31cca264-42c7-437e-8666-48f9ef393ed0")
		)
		(fp_poly
			(pts
				(xy -2.46 1.29) (xy -2.34 1.29) (xy -2.34 1.79) (xy -2.46 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "c959ccad-7a5e-41ee-8087-06cab4f02dbd")
		)
		(fp_poly
			(pts
				(xy -2.1595 -1.69) (xy -2.0395 -1.69) (xy -2.0395 -1.19) (xy -2.1595 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "eda8a48d-1c2e-45de-b237-f81d9cd6b6ca")
		)
		(fp_poly
			(pts
				(xy -1.8595 1.29) (xy -1.7395 1.29) (xy -1.7395 1.79) (xy -1.8595 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "d1a286d7-c5b8-4645-8880-f85c4af64a98")
		)
		(fp_poly
			(pts
				(xy -1.5595 -1.69) (xy -1.4395 -1.69) (xy -1.4395 -1.19) (xy -1.5595 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "d8bd7f92-eb5b-4e16-8489-5bd7c04ddcfa")
		)
		(fp_poly
			(pts
				(xy -1.26 1.29) (xy -1.14 1.29) (xy -1.14 1.79) (xy -1.26 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "5a5298f7-c4fc-43ee-9520-f87f2bf5e4a8")
		)
		(fp_poly
			(pts
				(xy -0.96 -1.69) (xy -0.84 -1.69) (xy -0.84 -1.19) (xy -0.96 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "1819e425-c2a2-407b-a217-891d968d9e1a")
		)
		(fp_poly
			(pts
				(xy -0.66 1.29) (xy -0.54 1.29) (xy -0.54 1.79) (xy -0.66 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "113e0cfe-415b-4b89-9866-daf314b02b68")
		)
		(fp_poly
			(pts
				(xy -0.36 -1.69) (xy -0.24 -1.69) (xy -0.24 -1.19) (xy -0.36 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "2458cc15-9112-461e-af8c-7c7057d5eece")
		)
		(fp_poly
			(pts
				(xy -0.06 1.29) (xy 0.06 1.29) (xy 0.06 1.79) (xy -0.06 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "5bb0c970-474c-4425-b2b6-a84d592d469d")
		)
		(fp_poly
			(pts
				(xy 0.24 -1.69) (xy 0.36 -1.69) (xy 0.36 -1.19) (xy 0.24 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "a5c754b4-25ac-4c2d-88c1-74c4e3b54cb9")
		)
		(fp_poly
			(pts
				(xy 0.54 1.29) (xy 0.66 1.29) (xy 0.66 1.79) (xy 0.54 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "878ca71f-351b-45f9-9223-72b6f6079d9b")
		)
		(fp_poly
			(pts
				(xy 0.8405 -1.69) (xy 0.9605 -1.69) (xy 0.9605 -1.19) (xy 0.8405 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "21b3f2b4-ea6f-4d66-8846-34c4d8edbe78")
		)
		(fp_poly
			(pts
				(xy 1.1405 1.29) (xy 1.2605 1.29) (xy 1.2605 1.79) (xy 1.1405 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "7c08aba7-e9c4-41d4-b520-67fca0ccd8c6")
		)
		(fp_poly
			(pts
				(xy 1.4405 -1.69) (xy 1.56 -1.69) (xy 1.56 -1.19) (xy 1.4405 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "2fa0e2de-3afa-46dd-b0c9-4d0c59b054c6")
		)
		(fp_poly
			(pts
				(xy 1.74 1.29) (xy 1.86 1.29) (xy 1.86 1.79) (xy 1.74 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "1f2a037d-c6a3-44a1-8e4a-507c34b6bfef")
		)
		(fp_poly
			(pts
				(xy 2.04 -1.69) (xy 2.16 -1.69) (xy 2.16 -1.19) (xy 2.04 -1.19)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "10e10888-e5c8-4049-ac21-076e09f391c8")
		)
		(fp_poly
			(pts
				(xy 2.34 1.29) (xy 2.46 1.29) (xy 2.46 1.79) (xy 2.34 1.79)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "a97c7fd6-327b-4616-b1b8-56090aeed201")
		)
		(fp_poly
			(pts
				(xy 3.04 0.54) (xy 3.16 0.54) (xy 3.16 1.54) (xy 3.04 1.54)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "ccaabbb7-9b0c-4275-95b8-65863a28e048")
		)
		(fp_line
			(start -3.3 -1.44)
			(end 3.3 -1.44)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "591376b6-c696-46ef-8bd3-becafc50bb6f")
		)
		(fp_line
			(start -3.3 1.96)
			(end -3.3 -1.44)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "9824b704-60eb-48db-93e2-e779e1b42694")
		)
		(fp_line
			(start 3.3 -1.44)
			(end 3.3 1.96)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "bcc8b540-97b3-42ad-899a-5b0a5561adae")
		)
		(fp_line
			(start 3.3 1.96)
			(end -3.3 1.96)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "d1019365-2f09-4fb4-93a3-6e4f3f5755ea")
		)
		(fp_poly
			(pts
				(xy -3.244567 1.937039) (xy -3.277039 1.904567) (xy -3.322961 1.904567) (xy -3.355433 1.937039)
				(xy -3.355433 1.982961) (xy -3.322961 2.015433) (xy -3.277039 2.015433) (xy -3.244567 1.982961)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.3")
			(uuid "f2f16d3e-3b0c-4a08-9c3b-541d88552801")
		)
		(pad "1" smd rect
			(at -2.4 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(J2-Pin_1)")
			(pinfunction "1")
			(pintype "unspecified")
			(uuid "276ed92d-0dba-4c0e-967a-d08a60c2c8bd")
		)
		(pad "2" smd rect
			(at -2.0995 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "Net-(J2-Pin_2)")
			(pinfunction "2")
			(pintype "unspecified")
			(uuid "59d44312-0fd0-47b3-ab70-1d1db68d06b7")
		)
		(pad "3" smd rect
			(at -1.7995 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "Net-(J2-Pin_3)")
			(pinfunction "3")
			(pintype "unspecified")
			(uuid "cdd83878-d1ee-427f-9dae-05c1fe5fca8f")
		)
		(pad "4" smd rect
			(at -1.4995 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(J2-Pin_4)")
			(pinfunction "4")
			(pintype "unspecified")
			(uuid "d955662f-06de-40fb-9714-2e0eebd2b9f6")
		)
		(pad "5" smd rect
			(at -1.2 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "Net-(J2-Pin_5)")
			(pinfunction "5")
			(pintype "unspecified")
			(uuid "4bb32eab-1775-4749-ae0e-76b3578b3776")
		)
		(pad "6" smd rect
			(at -0.9 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "Net-(J2-Pin_6)")
			(pinfunction "6")
			(pintype "unspecified")
			(uuid "1885837b-7f28-47ad-b3ae-598870dbb02e")
		)
		(pad "7" smd rect
			(at -0.6 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(J2-Pin_7)")
			(pinfunction "7")
			(pintype "unspecified")
			(uuid "01476762-5315-4d8f-a4d3-f4b5044c4e44")
		)
		(pad "8" smd rect
			(at -0.3 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(J2-Pin_8)")
			(pinfunction "8")
			(pintype "unspecified")
			(uuid "4fe115fa-341e-4c3d-8c3f-0d8d52faf2c5")
		)
		(pad "9" smd rect
			(at 0 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(J2-Pin_9)")
			(pinfunction "9")
			(pintype "unspecified")
			(uuid "73a8f19e-172a-4128-bda0-71b382ff0060")
		)
		(pad "10" smd rect
			(at 0.3 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(J2-Pin_10)")
			(pinfunction "10")
			(pintype "unspecified")
			(uuid "55742275-a992-409c-ac0e-11973caf632e")
		)
		(pad "11" smd rect
			(at 0.6 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Net-(J2-Pin_11)")
			(pinfunction "11")
			(pintype "unspecified")
			(uuid "e001d524-0612-4a77-9833-e66971441d2e")
		)
		(pad "12" smd rect
			(at 0.9005 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(J2-Pin_12)")
			(pinfunction "12")
			(pintype "unspecified")
			(uuid "b4e00aff-a774-424e-a67f-401e9972191e")
		)
		(pad "13" smd rect
			(at 1.2005 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(J2-Pin_13)")
			(pinfunction "13")
			(pintype "unspecified")
			(uuid "65ee113a-9c56-4656-bee0-357695bf5014")
		)
		(pad "14" smd rect
			(at 1.5005 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(J2-Pin_14)")
			(pinfunction "14")
			(pintype "unspecified")
			(uuid "67e2de1c-46e6-4eb8-ac8e-b6c86ca8da52")
		)
		(pad "15" smd rect
			(at 1.8 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "Net-(J2-Pin_15)")
			(pinfunction "15")
			(pintype "unspecified")
			(uuid "1a49c3df-4628-4c68-a7b8-06bfb27e8719")
		)
		(pad "16" smd rect
			(at 2.1 -1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Net-(J2-Pin_16)")
			(pinfunction "16")
			(pintype "unspecified")
			(uuid "a4d8f7be-bb6c-41ba-9af8-85d80e91bd1d")
		)
		(pad "17" smd rect
			(at 2.4 1.54)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/A_GND")
			(pinfunction "17")
			(pintype "unspecified")
			(uuid "17326a26-6c27-42c4-adec-c316e1d871ad")
		)
		(pad "18" smd rect
			(at 3.1 1.04)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/A_GND")
			(pinfunction "18")
			(pintype "unspecified")
			(uuid "19c38770-d3f5-4387-a47a-9abee14f7bcf")
		)
		(pad "19" smd rect
			(at -3.1 1.04)
			(size 0.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(uuid "c68627f0-aa15-4a26-8a29-40fe6aabb9a6")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/EASYEDA_MODELS/FPC-SMD_HCTL_HC-FPC-03-10-17RLTAG.step"
			(offset
				(xyz 0 -0.127 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "54bc34fd-fdf9-4f20-b777-8a3928f50b5c")
		(at 123.75 102.1 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "63c10352-b5e4-40bd-805f-d327d457ba61")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "85b0336d-9752-49fe-aa02-c532e32018b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "942102db-c718-4380-8fd0-90a70cd6e25a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e02faf87-1fe6-4812-9da7-58d340733654")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/be44b856-bd18-4c09-9ee0-04202caf4768")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c0ab450b-7f66-4529-86cf-8b418df09f35")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4b4be69-827b-4079-a6a8-91f115a01058")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8be24dac-bd02-41ef-a288-611daaf9ba62")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "530b1d62-2bbb-4b73-90ff-a28a49b6bb0a")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0198272b-7b0b-445c-b79e-0dd318eae1c6")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8325280-d671-491a-a1f9-16bd39fd091b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20f63b05-8245-4d72-a37f-e3c198f2fd67")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37055630-f5ae-4abe-b330-6caf8986c1b3")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "067cc643-efa2-434e-8314-45e226a69467")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb26fd9b-fe9c-4b10-8037-273ee61990a2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "323ad865-4fd2-4aa4-910f-145740e216ad")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/C_3V3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "26d86c0c-21fb-465d-b8fc-fe4a96f84281")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/GND")
			(pinfunction "2")
			(pintype "passive")
			(uuid "aff8cbe4-6e46-43d7-8309-1481d5d20a68")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EasyEDA_Lib:SOIC-8_L5.3-W5.3-P1.27-LS7.9-BL"
		(layer "F.Cu")
		(uuid "596fe854-7637-42a4-8d94-516eb0c9c399")
		(at 120.5 125.25 90)
		(property "Reference" "U2"
			(at -0.1845 -5.5 90)
			(layer "F.SilkS")
			(uuid "9ff82c56-966a-447d-b351-17695c1e026c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at -0.1845 5.5 90)
			(layer "F.Fab")
			(uuid "0fcbbac4-7277-41d0-8377-6e34da23fa4c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://item.szlcsc.com/datasheet/IS25LP128F-JBLE-TR/2154587.html"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "dc1152fa-b472-4f14-8192-70bb276e8196")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Interface:SPI Memory Size:128Mbit Clock Frequency:166MHz Voltage - Supply:2.3V~3.6V Voltage - Supply:2.3V~3.6V Standby Supply Current:8uA Program / Erase Cycles:100,000 Cycles Page Programming Time (Tpp):200us Block Erase Time(tBE):- Data Retention - TDR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ae2e2b45-055f-4915-914c-2927b03b9efd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "JLC_3DModel_Q" "15b9b546d7484425830d34b9890f9cc7"
			(at 0 0 90)
			(layer "Cmts.User")
			(hide yes)
			(uuid "8464f380-df47-47bb-b396-229682bf80c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "JLC_3D_Size" "7.9 5.28"
			(at 0 0 90)
			(layer "Cmts.User")
			(hide yes)
			(uuid "74ccf57a-4e13-496e-afa4-13d512cc75e6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer Part" "IS25LP128F-JBLE-TR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e639c024-0ddc-41b2-bc8b-14da8d79b9b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "ISSI(美国芯成)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd817f69-b206-4309-b9c1-45e537aaaa9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part" "C2063014"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2895b8d-a7d6-4601-b616-4c83b9230de4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier" "LCSC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "906fa916-b02c-4c74-9809-cad6d1280b70")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "LCSC Part Name" "具备166MHz多I/O SPI和四路I/O QPI DTR接口的128Mb串行闪存"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8cdb4916-05ce-45c7-a3b3-384af2cafaf6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/e8ff731c-cfde-4039-9d42-0d42592903d3")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(fp_line
			(start 2.65 -2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "9c756e66-3053-4d2d-b26b-810f2e6ae804")
		)
		(fp_line
			(start -2.65 -2.65)
			(end 2.65 -2.65)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "7c757750-2165-4a16-a5cf-be783fb8c3eb")
		)
		(fp_line
			(start 2.65 2.65)
			(end -2.65 2.65)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "f74b855c-baae-42c5-adae-a478b4e37ac3")
		)
		(fp_line
			(start -2.65 2.65)
			(end -2.65 -2.65)
			(stroke
				(width 0.15)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "99fd4a00-fb03-496f-9eb0-9b85fe54b9a2")
		)
		(fp_circle
			(center -2.794 3.302)
			(end -2.644 3.302)
			(stroke
				(width 0.3)
				(type default)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "e99d9d99-e531-434a-b4c4-fbd2495a303e")
		)
		(fp_circle
			(center -1.905 4.318)
			(end -1.705 4.318)
			(stroke
				(width 0.4)
				(type default)
			)
			(fill no)
			(layer "Dwgs.User")
			(uuid "3cae7c7b-d422-488b-aa5f-56525f8c8efa")
		)
		(fp_poly
			(pts
				(xy 1.705 -3.11) (xy 1.705 -3.95) (xy 2.105 -3.95) (xy 2.105 -3.11)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "1ff61b8a-19c0-499b-a9e8-77a2763b09a2")
		)
		(fp_poly
			(pts
				(xy 0.435 -3.11) (xy 0.435 -3.95) (xy 0.835 -3.95) (xy 0.835 -3.11)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "4c91f961-91bc-4af8-81d0-07bd62efcdd9")
		)
		(fp_poly
			(pts
				(xy -0.835 -3.11) (xy -0.835 -3.95) (xy -0.435 -3.95) (xy -0.435 -3.11)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "d0ca7167-e442-4448-a131-7497afdf492e")
		)
		(fp_poly
			(pts
				(xy -2.105 -3.11) (xy -2.105 -3.95) (xy -1.705 -3.95) (xy -1.705 -3.11)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "96d1b18b-0247-4385-8f8c-ca246b0d76ce")
		)
		(fp_poly
			(pts
				(xy 1.705 -2.64) (xy 1.705 -3.12) (xy 2.105 -3.12) (xy 2.105 -2.64)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "9b1c36e4-f670-4191-959b-b7bc30bd1cd7")
		)
		(fp_poly
			(pts
				(xy 0.435 -2.64) (xy 0.435 -3.12) (xy 0.835 -3.12) (xy 0.835 -2.64)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "5547cd76-f498-4808-85d8-002b67ef99f9")
		)
		(fp_poly
			(pts
				(xy -0.835 -2.64) (xy -0.835 -3.12) (xy -0.435 -3.12) (xy -0.435 -2.64)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "3e957fe6-fd6a-4703-b513-f42eeedd3957")
		)
		(fp_poly
			(pts
				(xy -2.105 -2.64) (xy -2.105 -3.12) (xy -1.705 -3.12) (xy -1.705 -2.64)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "adae2ab7-5f81-446e-b7d9-e73c155a7f08")
		)
		(fp_poly
			(pts
				(xy 1.705 3.12) (xy 1.705 2.64) (xy 2.105 2.64) (xy 2.105 3.12)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "a3cd1967-c66c-4e8d-a545-e4f17b170adc")
		)
		(fp_poly
			(pts
				(xy 0.435 3.12) (xy 0.435 2.64) (xy 0.835 2.64) (xy 0.835 3.12)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "e8dd115e-2093-4e79-a614-9dffafa0f49a")
		)
		(fp_poly
			(pts
				(xy -0.835 3.12) (xy -0.835 2.64) (xy -0.435 2.64) (xy -0.435 3.12)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "b2fa7f94-3990-46e5-94de-86218ec730d0")
		)
		(fp_poly
			(pts
				(xy -2.105 3.12) (xy -2.105 2.64) (xy -1.705 2.64) (xy -1.705 3.12)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "14568343-dd29-48d3-bd35-631150fd27c4")
		)
		(fp_poly
			(pts
				(xy 1.705 3.95) (xy 1.705 3.11) (xy 2.105 3.11) (xy 2.105 3.95)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "fcc40a8d-3c8d-4a07-be66-adcf91d4b27b")
		)
		(fp_poly
			(pts
				(xy 0.435 3.95) (xy 0.435 3.11) (xy 0.835 3.11) (xy 0.835 3.95)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "80c78b56-75fc-46a7-ae6f-59b3be383481")
		)
		(fp_poly
			(pts
				(xy -0.835 3.95) (xy -0.835 3.11) (xy -0.435 3.11) (xy -0.435 3.95)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "0a1226b2-923e-4470-ae93-6a37974d339b")
		)
		(fp_poly
			(pts
				(xy -2.105 3.95) (xy -2.105 3.11) (xy -1.705 3.11) (xy -1.705 3.95)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.1")
			(uuid "030c07db-ab6f-4de7-81e5-1b2445e27e11")
		)
		(fp_line
			(start 2.65 -2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "3e381b82-c78e-4ce3-ab04-2ca2b19ebf4d")
		)
		(fp_line
			(start -2.65 -2.65)
			(end 2.65 -2.65)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "38973475-266f-4b78-8858-03756437eb33")
		)
		(fp_line
			(start 2.65 2.65)
			(end -2.65 2.65)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "b2c37225-c25c-4a79-80f2-376eda1fa4be")
		)
		(fp_line
			(start -2.65 2.65)
			(end -2.65 -2.65)
			(stroke
				(width 0.051)
				(type default)
			)
			(layer "User.2")
			(uuid "f99262ae-c9fb-4a17-8847-aa33b59145d8")
		)
		(fp_poly
			(pts
				(xy -2.594567 3.927039) (xy -2.627039 3.894567) (xy -2.672961 3.894567) (xy -2.705433 3.927039)
				(xy -2.705433 3.972961) (xy -2.672961 4.005433) (xy -2.627039 4.005433) (xy -2.594567 3.972961)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "User.3")
			(uuid "0ded4a70-5298-4179-9605-d69cc96d56e2")
		)
		(pad "1" smd rect
			(at -1.905 3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/FLASH_CS")
			(pinfunction "CE#")
			(pintype "unspecified")
			(uuid "77e97ebd-6a7a-4ba0-bb08-b15e2c33b89c")
		)
		(pad "2" smd rect
			(at -0.635 3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/SPI_MISO")
			(pinfunction "SO/IO1")
			(pintype "unspecified")
			(uuid "ee1139c9-4091-4484-bdb7-a5b6cb83e259")
		)
		(pad "3" smd rect
			(at 0.635 3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/C_3V3")
			(pinfunction "WP#/IO2")
			(pintype "unspecified")
			(uuid "7c403430-c24c-4121-abd3-5f82b729679d")
		)
		(pad "4" smd rect
			(at 1.905 3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "unspecified")
			(uuid "b581336b-5033-48e2-9d48-d3cab7b143f7")
		)
		(pad "5" smd rect
			(at 1.905 -3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/SPI_MOSI")
			(pinfunction "SI/IO0")
			(pintype "unspecified")
			(uuid "4990a0da-220f-478a-bfde-0ff9477796de")
		)
		(pad "6" smd rect
			(at 0.635 -3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/SPI_SCK")
			(pinfunction "SCK")
			(pintype "unspecified")
			(uuid "bf559a69-48fe-4bed-a776-18f3f528064f")
		)
		(pad "7" smd rect
			(at -0.635 -3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/C_3V3")
			(pinfunction "HOLD#/RESET#/IO3")
			(pintype "unspecified")
			(uuid "0b84c073-951f-41e4-89ff-00e7215cba04")
		)
		(pad "8" smd rect
			(at -1.905 -3.9 90)
			(size 0.7 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/C_3V3")
			(pinfunction "VCC")
			(pintype "unspecified")
			(uuid "1b893233-ba78-4bcb-8e5a-ac674c25728d")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/EASYEDA_MODELS/SOIC-8_L5.3-W5.3-P1.27-LS7.9-BL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "7c96a877-bbc7-4fcd-a04e-96040626df96")
		(at 118.8 120.25 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "424fa8a5-691c-45d1-b543-afa674db1f6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "66e5674c-ab21-44b1-b28d-2ea0fe034bde")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c843b2f-5d94-4175-8196-ed765d43e69b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d1d62885-6fbc-4cc0-931b-d43bf27b4840")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/4ea7caff-53f9-4c00-bf01-2c0cfc1ebd9c")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97ac5bb3-65d2-4821-acc6-811a228fa888")
		)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5f75370-6cde-4680-91d3-495c35b5c61d")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3bb202b8-b5db-4bdc-9af1-4b8132702feb")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b55fd0c-3709-4669-a304-559162e4a0ba")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c64dded4-f497-432a-b1e5-cf2f0c7f038c")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "434f8d5a-943f-4f63-9fce-846b39bbdbbd")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e135f86-c1eb-4f85-889c-15c65850d3ac")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1dccc864-e48f-4fd1-8bd8-12e86b805017")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c3d9f29-ae13-4fad-a6c7-79bbe349bc49")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0edf07f-fe11-4cb5-a6b1-0cff8111dcc8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d711eddb-c2ef-49c2-aedc-e359028b032f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/C_3V3")
			(pinfunction "1")
			(pintype "passive")
			(uuid "05c4eb02-2824-4c5e-babd-eb7815cc2475")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/GND")
			(pinfunction "2")
			(pintype "passive")
			(uuid "8bedec4c-fcb9-4e5b-b5fe-1df2361f5bf2")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:XIAO-nRF52840-DIP"
		(layer "F.Cu")
		(uuid "80914990-c477-4ae5-bdff-601c74402029")
		(at 111.38 106.62 90)
		(property "Reference" "U3"
			(at -0.025 -10.275 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "b3a5645f-dcc9-4401-ab7f-1fc4927414f7")
			(effects
				(font
					(size 0.635 0.635)
					(thickness 0.1016)
				)
			)
		)
		(property "Value" "XIAO-nRF52840-DIP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "a798ee2b-b550-4a2f-bb66-760a91b87fa1")
			(effects
				(font
					(size 0.635 0.635)
					(thickness 0.1016)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e306a4d8-c125-409b-8af3-7e7e6e093393")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5b3d61c5-ff04-477a-85f3-e3ca0f2d4ad0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/fe1b6661-12b7-4ecc-bcbc-62703a98c889")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -8.509 -8.89)
			(end 8.636 -8.89)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd0092d7-8327-444a-9677-329a95386666")
		)
		(fp_line
			(start -10.414 -6.985)
			(end -10.414 6.985)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4ada586-7109-457d-a828-a3d23fdd18ce")
		)
		(fp_line
			(start 10.541 -4.495)
			(end 11.551272 -4.491272)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e1d4d89-2212-4c3f-bac9-58c326257b1b")
		)
		(fp_line
			(start 12.051 -3.991272)
			(end 12.051 4.004)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b7cd843-c3cf-4641-a3c4-bf0246187b60")
		)
		(fp_line
			(start 11.551 4.504)
			(end 10.541 4.504)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf745b9d-e176-471e-a408-4dd75d3e899f")
		)
		(fp_line
			(start 10.541 6.985)
			(end 10.541 -6.985)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2bc327cd-8b03-4b85-9284-9179a6320f34")
		)
		(fp_line
			(start 10.541 6.985)
			(end 10.541 -6.985)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b7858e1-d887-48e6-8531-dab877098131")
		)
		(fp_line
			(start -8.509 8.89)
			(end 8.636 8.89)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c359d81-15d8-4d8f-868a-cc03e4a6a374")
		)
		(fp_arc
			(start 8.636 -8.89)
			(mid 9.983038 -8.332038)
			(end 10.541 -6.985)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2bf45a28-198b-4b2f-bc7f-1ba2bcb08451")
		)
		(fp_arc
			(start -10.414 -6.985)
			(mid -9.856038 -8.332038)
			(end -8.509 -8.89)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75a3c9c2-fd6f-468f-9382-fb0cf85bf479")
		)
		(fp_arc
			(start 11.551272 -4.491272)
			(mid 11.904644 -4.344724)
			(end 12.051 -3.991272)
			(stroke
				(width 0.127)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "8301f29f-bb84-46fa-8b99-953e6e5d7564")
		)
		(fp_arc
			(start 12.051 4.004)
			(mid 11.904524 4.357524)
			(end 11.551 4.504)
			(stroke
				(width 0.127)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "f594aecf-5189-4fb2-b18c-85e9bafe89ad")
		)
		(fp_arc
			(start 10.541 6.985)
			(mid 9.983038 8.332038)
			(end 8.636 8.89)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38c49176-e105-4ae5-8f90-ce3e34b5f431")
		)
		(fp_arc
			(start -8.509 8.89)
			(mid -9.856038 8.332038)
			(end -10.414 6.985)
			(stroke
				(width 0.127)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8489ddc8-15c0-4c65-9feb-222092d7cfca")
		)
		(fp_circle
			(center 10.4 -8.85)
			(end 10.654 -8.85)
			(stroke
				(width 0.5)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "6062c251-e0e8-4d09-a651-2de1055b4243")
		)
		(fp_circle
			(center 9.52 -7.707)
			(end 9.774 -7.707)
			(stroke
				(width 0.5)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "2336b0db-f208-462e-93cf-43be34a169d0")
		)
		(fp_rect
			(start -10.425 -8.9)
			(end 10.55 8.9)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "6496eb91-0be3-4c6b-bd62-420a41c177e9")
		)
		(fp_rect
			(start -10.425 -8.9)
			(end 10.55 8.9)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "89a2a3ac-648f-453c-a0d9-03cb38801f97")
		)
		(fp_circle
			(center 9.526 -7.704)
			(end 9.78 -7.704)
			(stroke
				(width 0.5)
				(type solid)
			)
			(fill yes)
			(layer "F.Fab")
			(uuid "0c280245-f77b-4f64-a096-b3dba48b0954")
		)
		(pad "1" smd roundrect
			(at 7.62 -8.455 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 6 "/C_BTN1")
			(pinfunction "P0.02_A0_D0")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "f418c120-011a-4229-82d4-99c8dba9b5e2")
		)
		(pad "1" thru_hole circle
			(at 7.62 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/C_BTN1")
			(pinfunction "P0.02_A0_D0")
			(pintype "passive")
			(uuid "1f12616a-2b4a-4a79-8974-8b0dfc806b06")
		)
		(pad "2" smd roundrect
			(at 5.08 -8.455 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 16 "/C_BTN2")
			(pinfunction "P0.03_A1_D1")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "5ca1bf2b-9380-44a0-8d1a-9d05a45127c1")
		)
		(pad "2" thru_hole circle
			(at 5.08 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/C_BTN2")
			(pinfunction "P0.03_A1_D1")
			(pintype "passive")
			(uuid "b9077111-3ede-4a1f-93bc-8a2024a4db87")
		)
		(pad "3" smd roundrect
			(at 2.54 -8.455 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 5 "/C_BTN3")
			(pinfunction "P0.28_A2_D2")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "9673498f-7902-4bb6-a905-bd51b4786c61")
		)
		(pad "3" thru_hole circle
			(at 2.54 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/C_BTN3")
			(pinfunction "P0.28_A2_D2")
			(pintype "passive")
			(uuid "4332b759-58d5-4835-8078-d37842f20ded")
		)
		(pad "4" smd roundrect
			(at 0 -8.455 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 11 "/C_BTN4")
			(pinfunction "P0.29_A3_D3")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "a2436725-9824-491d-a7c4-d18e066cc282")
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/C_BTN4")
			(pinfunction "P0.29_A3_D3")
			(pintype "passive")
			(uuid "daa4dfaf-030e-4f9a-adcf-ce386abe2e07")
		)
		(pad "5" smd roundrect
			(at -2.54 -8.455 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 21 "/FLASH_CS")
			(pinfunction "P0.04_A4_D4_SDA")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "a2c0fd9e-cfd6-43db-ba94-5feb4fc77bf0")
		)
		(pad "5" thru_hole circle
			(at -2.54 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/FLASH_CS")
			(pinfunction "P0.04_A4_D4_SDA")
			(pintype "passive")
			(uuid "abc1fb9a-de81-4d9c-bf7c-228d29987d16")
		)
		(pad "6" smd roundrect
			(at -5.08 -8.455 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 20 "/AUDIO_PWM")
			(pinfunction "P0.05_A5_D5_SCL")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "dcfd230b-1741-4269-848a-ffce73a9c056")
		)
		(pad "6" thru_hole circle
			(at -5.08 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/AUDIO_PWM")
			(pinfunction "P0.05_A5_D5_SCL")
			(pintype "passive")
			(uuid "5ae6d46d-91c9-4ad4-93fa-f4a307b04650")
		)
		(pad "7" smd roundrect
			(at -7.62 -8.455 180)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 27 "unconnected-(U3-P1.11_D6_TX-Pad7)")
			(pinfunction "P1.11_D6_TX")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "7985f736-a1ef-41ee-9980-df8c0757c88d")
		)
		(pad "7" thru_hole circle
			(at -7.62 -7.62 180)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(U3-P1.11_D6_TX-Pad7)")
			(pinfunction "P1.11_D6_TX")
			(pintype "passive")
			(uuid "138859d1-3dbe-48be-a327-a28796c9f972")
		)
		(pad "8" thru_hole circle
			(at -7.62 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(U3-P1.12_D7_RX-Pad8)")
			(pinfunction "P1.12_D7_RX")
			(pintype "passive")
			(uuid "93afc882-acec-4829-be86-2d9c32b6aaa1")
		)
		(pad "8" smd roundrect
			(at -7.62 8.455)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 28 "unconnected-(U3-P1.12_D7_RX-Pad8)")
			(pinfunction "P1.12_D7_RX")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "5a7c4520-c241-48ce-9628-6dc8dc0642e4")
		)
		(pad "9" thru_hole circle
			(at -5.08 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/SPI_SCK")
			(pinfunction "P1.13_D8_SCK")
			(pintype "passive")
			(uuid "30ac77ed-de8d-49e4-a6f7-e517bbd1c93c")
		)
		(pad "9" smd roundrect
			(at -5.08 8.455)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 24 "/SPI_SCK")
			(pinfunction "P1.13_D8_SCK")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "13805602-bcee-47d2-9b08-61b4faf641eb")
		)
		(pad "10" thru_hole circle
			(at -2.54 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/SPI_MISO")
			(pinfunction "P1.14_D9_MISO")
			(pintype "passive")
			(uuid "12bdda37-d984-4b4b-8009-7f5e98e89d5f")
		)
		(pad "10" smd roundrect
			(at -2.54 8.455)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 25 "/SPI_MISO")
			(pinfunction "P1.14_D9_MISO")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "fa7a878f-dede-4c83-8fed-04871674ef17")
		)
		(pad "11" thru_hole circle
			(at 0 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/SPI_MOSI")
			(pinfunction "P1.15_D10_MOSI")
			(pintype "passive")
			(uuid "87f0d054-b2e4-45f4-b7f1-b69d3e1e7a9e")
		)
		(pad "11" smd roundrect
			(at 0 8.455)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 23 "/SPI_MOSI")
			(pinfunction "P1.15_D10_MOSI")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "15c6a06b-e2f2-4bc2-ac93-e2808f20dbd5")
		)
		(pad "12" thru_hole circle
			(at 2.54 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/C_3V3")
			(pinfunction "3V3")
			(pintype "passive")
			(uuid "1873fab1-b528-4c9c-bd77-c546f2a8ff69")
		)
		(pad "12" smd roundrect
			(at 2.54 8.455)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 3 "/C_3V3")
			(pinfunction "3V3")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "5bfba32c-f500-4ace-945d-2d72d8aa269e")
		)
		(pad "13" thru_hole circle
			(at 5.08 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
			(uuid "dda3db8e-f80c-4993-9de5-372f82becdb2")
		)
		(pad "13" smd roundrect
			(at 5.08 8.455)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "9b1142a1-dc8c-4155-a5fb-e4e6287e99ec")
		)
		(pad "14" thru_hole circle
			(at 7.62 7.62)
			(size 1.524 1.524)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(U3-VBUS-Pad14)")
			(pinfunction "VBUS")
			(pintype "passive")
			(uuid "1ba69f05-3eee-4c5b-9799-370f9178a0dd")
		)
		(pad "14" smd roundrect
			(at 7.62 8.455)
			(size 2.432 1.524)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1)
			(net 26 "unconnected-(U3-VBUS-Pad14)")
			(pinfunction "VBUS")
			(pintype "passive")
			(thermal_bridge_angle 45)
			(uuid "03d93bd9-a2d6-4d78-bc0f-db2c13152330")
		)
		(embedded_fonts no)
		(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-nRF52840 v15.step"
			(hide yes)
			(offset
				(xyz -1.778 -6.096 0.381)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeeduino XIAO SAMD21 v4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO RP2040 v26.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
		(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO-ESP32-C3.step"
			(hide yes)
			(offset
				(xyz -1.7018 -6.096 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-ESP32S3 v2.step"
			(hide yes)
			(offset
				(xyz -1.778 -6.1722 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:Texas_R-PDSO-G6"
		(layer "F.Cu")
		(uuid "91fbc178-a689-4193-b8f8-95eb88f5c09b")
		(at 123.85 107.15 180)
		(descr "R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf")
		(tags "R-PDSO-G6 SC-70-6")
		(property "Reference" "U1"
			(at 0.5 -1.4 0)
			(layer "F.SilkS")
			(uuid "016f9e05-ce3b-4584-beb5-3de0c1373a37")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS61220DCK"
			(at 0 2 0)
			(layer "F.Fab")
			(uuid "ce995dc5-211e-4bec-9145-5263356f8196")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps61220.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ce8a2590-a38a-43b1-9cfa-eda3f36e7a81")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "400 mA Step-Up Converter, Adjustable Output Voltage, 0.7-5.5V Input Voltage, SC-70"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a1b8d2f9-eb66-404b-959b-2b288a4e5313")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Texas*R*PDSO*G6*")
		(path "/7891744c-4198-4103-8ab8-7ee73d24d5de")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.7 1.16)
			(end 0.7 1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f287169b-fe4b-405d-a528-2f5208af8512")
		)
		(fp_line
			(start -0.7 -1.16)
			(end 0.7 -1.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4fe8240-824e-4bd9-95cb-2b51c94b8d56")
		)
		(fp_poly
			(pts
				(xy -1.12 -1.11) (xy -1.36 -1.44) (xy -0.88 -1.44) (xy -1.12 -1.11)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "0f1b85f3-08a5-41ca-924e-9ec4691bcf3f")
		)
		(fp_line
			(start 1.6 1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e29d3c4-2cd7-4586-9797-b5ec76977922")
		)
		(fp_line
			(start -1.6 1.4)
			(end 1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2f2981b-60f8-41a4-98db-14b4a9fe6979")
		)
		(fp_line
			(start -1.6 -1.4)
			(end 1.6 -1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cb53e3b9-4c0f-40ce-8b37-35fa0edf6593")
		)
		(fp_line
			(start -1.6 -1.4)
			(end -1.6 1.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "115023dd-1719-4da3-8369-537818b150b8")
		)
		(fp_line
			(start 0.675 1.1)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "feeb9aa6-7815-4b05-a9b8-44bfdf244603")
		)
		(fp_line
			(start 0.675 -1.1)
			(end 0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a8afd95-8358-4447-adb9-9c0cf8763ae7")
		)
		(fp_line
			(start 0.675 -1.1)
			(end -0.175 -1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "55323577-b9ad-4eee-bc87-913739b1a42a")
		)
		(fp_line
			(start -0.175 -1.1)
			(end -0.675 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68ab3e0f-63fc-4a2f-b0e4-6c9c4b56fa95")
		)
		(fp_line
			(start -0.675 -0.6)
			(end -0.675 1.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "254ec125-dadf-4a2e-ac69-0c8c0d0bb924")
		)
		(fp_text user "${REFERENCE}"
			(at 0.5 0.85 90)
			(layer "F.Fab")
			(uuid "4a325f3a-4780-44c5-b878-4ce430df386a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.075)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.1 -0.65 180)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/C_VBAT")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "75f2dbaa-e0a8-4b9e-8f81-bde588274e5d")
		)
		(pad "2" smd roundrect
			(at -1.1 0 180)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "unconnected-(U1-FB-Pad2)")
			(pinfunction "FB")
			(pintype "input")
			(uuid "24997886-2564-4e72-a896-06ad506a85e7")
		)
		(pad "3" smd roundrect
			(at -1.1 0.65 180)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "6e2a3f19-3505-4e43-8f52-4dc88048b8d9")
		)
		(pad "4" smd roundrect
			(at 1.1 0.65 180)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/C_3V3")
			(pinfunction "VOUT")
			(pintype "power_out")
			(uuid "d0cca909-4368-43f5-aa14-3047c2c10205")
		)
		(pad "5" smd roundrect
			(at 1.1 0 180)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/BOOST_SW")
			(pinfunction "L")
			(pintype "power_in")
			(uuid "968f297c-7d8d-4976-87b3-dfc86dad5bb2")
		)
		(pad "6" smd roundrect
			(at 1.1 -0.65 180)
			(size 0.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/C_VBAT")
			(pinfunction "EN")
			(pintype "input")
			(uuid "1b16815d-759e-492f-a026-da324da489c1")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:A16N_cast"
		(layer "F.Cu")
		(uuid "93eb03c1-03c9-4598-a9d5-3a34276c2385")
		(at 107.75 134.445 90)
		(property "Reference" "J2"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "77211aaa-5b65-48ff-8fa2-001b09569fc9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(property "Value" "SOP16-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b67f5c19-83f7-40b2-96b0-7df50e6edb4c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "1685da6c-0ca2-4bb1-8f11-2600a9135fa9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x16, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "ea713ac5-23a1-4b49-b05e-7bea3b5ca6cc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/aecf1cc8-2ce6-4443-93d1-69e69d4737e5")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(fp_line
			(start -5.5 -2)
			(end 5.5 -2)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "Edge.Cuts")
			(uuid "6c3e2386-8a74-4616-a67b-418aef79a7b0")
		)
		(fp_line
			(start 5.5 2)
			(end -5.5 2)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "Edge.Cuts")
			(uuid "67cbb35a-f5f5-46f1-99d2-565c2409a074")
		)
		(pad "1" thru_hole circle
			(at -4.445 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "aa4f5818-d9ad-4bbe-9288-c0c6ca16fc2f")
		)
		(pad "2" thru_hole circle
			(at -3.175 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "4694aeda-4272-4686-baf2-8c74ce3e1e9b")
		)
		(pad "3" thru_hole circle
			(at -1.905 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "52c291cf-f8be-4bf4-8b53-59a0bd2d4d75")
		)
		(pad "4" thru_hole circle
			(at -0.635 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "25617bb2-247e-4ea3-abd8-9b18cd39ff09")
		)
		(pad "5" thru_hole circle
			(at 0.635 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "72d8693b-d61a-425f-8b87-089ff8d66638")
		)
		(pad "6" thru_hole circle
			(at 1.905 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "c0e5c9aa-5667-404b-89b8-40233072d7ca")
		)
		(pad "7" thru_hole circle
			(at 3.175 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "dcf9908d-8120-4f7c-abdd-3b63b9029e8a")
		)
		(pad "8" thru_hole circle
			(at 4.445 -2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "476fbfc0-4ec9-4bed-a7b9-25f83353f7f6")
		)
		(pad "9" thru_hole circle
			(at 4.445 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(J2-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "e0d9bc83-0a32-4cec-a57a-13c058b8c968")
		)
		(pad "10" thru_hole circle
			(at 3.175 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
			(uuid "349096e4-17e4-4354-9de7-deb6e77f3123")
		)
		(pad "11" thru_hole circle
			(at 1.905 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(J2-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
			(uuid "68b8f0d0-a6f4-4043-961e-0168f94e5387")
		)
		(pad "12" thru_hole circle
			(at 0.635 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(J2-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
			(uuid "25a33dac-4abf-49f0-b60a-576a46a7b7dd")
		)
		(pad "13" thru_hole circle
			(at -0.635 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(J2-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
			(uuid "c0897792-c237-4c0c-8e6f-4db83d15a5a2")
		)
		(pad "14" thru_hole circle
			(at -1.905 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(J2-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
			(uuid "aef9903c-0dac-4e7f-8bf3-5509f99cc26b")
		)
		(pad "15" thru_hole circle
			(at -3.175 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J2-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
			(uuid "922ed25d-163b-4c40-9019-5f0cbda904b8")
		)
		(pad "16" thru_hole circle
			(at -4.445 2 90)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(J2-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
			(uuid "1a068291-d7e1-43a4-9bbf-3790d0ad28a7")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "9da477d3-786c-47b9-8ecb-760e22cd855b")
		(at 123.75 116.2 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(uuid "90fdaed2-29f8-491c-8160-35896ce81cf4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(uuid "700c6a85-af00-4e6d-a5bf-fcd7ceedc6f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "86013115-1605-4fbd-8e75-1995d2db3804")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "9cb12452-7d6b-4147-b40e-9e02e74eda7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/d225c3fa-9586-478d-a854-6d14dbaa4bfd")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ced85280-0f86-497e-864d-257a3e5b2960")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "073216fb-cf90-412e-bcc8-05462559db8b")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "42931d6c-509a-4ef1-8c77-6498888ff821")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e557470e-1a87-4d70-a6ac-9e53dbd52685")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "916ea203-0207-4ca4-93c3-350e0b002f5b")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47000ee5-3201-42c7-bcfc-b3fa34f4e139")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1651c36f-ba19-4197-b30e-fbebdb70d0ad")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "878ec201-c7d0-4c42-9790-1752d0561b00")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc17810a-608c-4450-b613-e22e7a78885e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31d14474-4294-440f-84c7-3d5f24b66c82")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "5caab575-1945-48b4-b737-87a2df97644a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/C_VBAT")
			(pinfunction "1")
			(pintype "passive")
			(uuid "aa2540dc-6714-4c7b-9228-56a45e40d8a7")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/GND")
			(pinfunction "2")
			(pintype "passive")
			(uuid "8d78901e-1f07-4db9-be0f-e982dd0397cd")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "e4096db0-31a3-4cfb-a1e6-33f9e044979b")
		(at 112.3 120)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
			(uuid "a84f2d7f-0348-41c3-9b47-28372a2e3873")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10nF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(uuid "a7ed58f8-5399-4a62-97b4-125a56050e7f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6a6bb4d2-9d07-4414-8776-fae627dd73c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3a2a948-9d48-4d1c-b062-e7f0c1db6753")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/16705866-bee7-4f26-a10e-6f7bfbff4c09")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261252 -0.735)
			(end 0.261252 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76bb73e6-fd90-4f56-aab5-cb9c9439fe79")
		)
		(fp_line
			(start -0.261252 0.735)
			(end 0.261252 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73e14c07-d8d8-4bcf-a4a7-728decdaa93a")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7535fde1-c552-4802-a1b0-96f38be78ce6")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f1574e2-45ae-4a64-a63e-fb2750620d41")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9dc78e1-0b1f-4bc2-a626-e7516a908bea")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c63028f-70f0-4756-af9c-f5df57a7e414")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b74bbf8-692b-4a74-ad65-7f9d5aec64f2")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c215f692-696c-4326-95f1-c94c6d9a1c78")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23d3b839-c7a3-4398-b074-8ceae6fdeb57")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f53b3b6f-1b49-4873-a4b6-53a90570203f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "50522637-ab98-420e-97c9-6ebe42259ed2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AUDIO_OUT")
			(pinfunction "1")
			(pintype "passive")
			(uuid "61c6f319-5b57-472e-acd3-93a676f39b78")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/GND")
			(pinfunction "2")
			(pintype "passive")
			(uuid "49f5d48f-8e1f-489b-9e73-4ab9853a165c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "f1d3a006-c0ec-4edf-85f1-f1226faaec2d")
		(at 108.5125 120)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "894d9106-a23d-4265-ae37-53c8d3341616")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.7K"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "e403449f-203f-4ae1-9e38-e70523682981")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "16c3d369-0f8d-4a66-8af5-95e6431c3a15")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b559384f-509a-41b1-b8a0-b8c5d92c8dc5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/a658da19-5644-4160-b300-be8c7c773405")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b47675ad-b4bd-4cbe-a916-eb5336a16a6d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0359e325-c08f-4f67-a094-476ea5f7a601")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca594cf1-117f-41b6-aea0-3e487772b4ca")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a4b11f1e-616e-4323-bf4b-fb22fabd85f3")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fce2abe1-6b9f-45c6-b45e-663eea882170")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d58dbc3d-47f7-4efa-9bef-a5c9e997fa81")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25fd39f3-6905-4e52-bf21-16dca240ed33")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a95cd09-ccd7-4f28-b28d-3aa336db39cb")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d9ca190-b9ca-4a92-936a-1d0f66d9ae93")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "593680a8-d56d-4e0a-8250-435f1b2b9ff4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5f309e07-48b5-4684-abe7-e63395cd7be8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 20 "/AUDIO_PWM")
			(pinfunction "1")
			(pintype "passive")
			(uuid "404305c7-5fc8-4f03-b537-bc2de8b48fe2")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 4 "/AUDIO_OUT")
			(pinfunction "2")
			(pintype "passive")
			(uuid "4a280e60-c9b1-405f-b1b2-9aa9399f381c")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "f7f360e7-11f5-4158-a234-e75c1d3cfa62")
		(at 122.9125 120.25 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "4d7c07af-ff00-4b48-b204-b3091b3a826f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10K"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ba0dffcf-dfe0-41ec-b9dc-5120f42b17dd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c373a6f3-f2f7-42bc-9cdc-cd69161f894d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e105c95-7a96-4aaf-a739-44e3d0da91ab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/696b8ca8-97f4-4851-97cc-70c56c8f54f5")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "74ce5f45-42ca-48a8-ad05-03249bac0624")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d45bb0fa-c3b9-4620-9665-cc7921de61ec")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5557f7d6-7339-46d1-b5f2-7288c3429bdf")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7530ed49-e34a-4b93-ac9c-775962163f14")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ed9b64ff-9be1-4db2-9521-e65efd8cc6c0")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c737a3d-80ce-484a-8bcb-02981475c677")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72fcd0de-d091-4067-9274-94e49443850a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73618937-a4de-4689-ba0d-1a4fb1911ccc")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96e2871b-e17e-473a-9fc4-cac91058ffe2")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f4bdec0-4c6b-48ae-80ed-1574610375a3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7ec36149-665f-49e9-845f-d100ac87c875")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 21 "/FLASH_CS")
			(pinfunction "1")
			(pintype "passive")
			(uuid "fcc0ead4-e6c8-4af6-89d1-4413912c36e2")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 3 "/C_3V3")
			(pinfunction "2")
			(pintype "passive")
			(uuid "03085373-55d6-48ad-a078-bab098f1a946")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:A16N_cast"
		(layer "B.Cu")
		(uuid "ae99d7f5-b180-4dfb-b6a2-cfcf3a91ec1a")
		(at 118 134.445 -90)
		(property "Reference" "J1"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "d16ce3c3-3e87-43a0-bbc6-940e768ee51c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(property "Value" "SOP16-3"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "4f43c2a8-3bcf-47f9-98c3-afe2bc5f53ce")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5b03e196-52f7-41ad-bce9-41fa73314a8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Generic connector, single row, 01x16, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "88811052-074d-44d5-89d2-1b35f945f9d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/c6236fa0-f3ae-409f-8b42-1a96fca23a4e")
		(sheetname "/")
		(sheetfile "baby-mobile-v5.kicad_sch")
		(fp_line
			(start -5.5 2)
			(end 5.5 2)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "Edge.Cuts")
			(uuid "0c3b831a-aade-4b2d-8a44-e5670be6195c")
		)
		(fp_line
			(start 5.5 -2)
			(end -5.5 -2)
			(stroke
				(width 0.05)
				(type default)
			)
			(layer "Edge.Cuts")
			(uuid "d6cce824-2cd5-4461-b8cb-99a9db313f98")
		)
		(pad "1" thru_hole circle
			(at -4.445 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f5eafaee-5a62-4e10-b1da-cf04df229073")
		)
		(pad "2" thru_hole circle
			(at -3.175 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "383fbc77-ad55-4965-b55e-9a1546e3747b")
		)
		(pad "3" thru_hole circle
			(at -1.905 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "a365d3a4-c79a-47dc-ad5d-0e3e6672a005")
		)
		(pad "4" thru_hole circle
			(at -0.635 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "fd1d49e9-0cd2-4c33-ad78-a73d4a0e02c8")
		)
		(pad "5" thru_hole circle
			(at 0.635 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "a4414473-a9d3-4e5b-898f-af82b020f65e")
		)
		(pad "6" thru_hole circle
			(at 1.905 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "8c47d681-d344-4554-bf00-0d7cc02e4789")
		)
		(pad "7" thru_hole circle
			(at 3.175 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "7fbdf851-b4ce-457f-946c-dc0919027516")
		)
		(pad "8" thru_hole circle
			(at 4.445 2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "ad516b60-84c6-4d2f-9b14-24aebd186989")
		)
		(pad "9" thru_hole circle
			(at 4.445 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "81f476fc-d322-47fa-bb04-c5e0093ea14f")
		)
		(pad "10" thru_hole circle
			(at 3.175 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
			(uuid "550fbdae-a3c5-4359-aab5-bde2b3557319")
		)
		(pad "11" thru_hole circle
			(at 1.905 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J1-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
			(uuid "e527c700-236e-4d28-824a-1af96d271546")
		)
		(pad "12" thru_hole circle
			(at 0.635 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
			(uuid "74e24333-209b-4d15-82af-a334e34c7b15")
		)
		(pad "13" thru_hole circle
			(at -0.635 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J1-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
			(uuid "85ee0f03-9394-4f23-93fe-03d6d1db93ef")
		)
		(pad "14" thru_hole circle
			(at -1.905 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
			(uuid "edb2d893-fc0a-4089-a798-59adcf4073a9")
		)
		(pad "15" thru_hole circle
			(at -3.175 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J1-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
			(uuid "bcc790eb-a841-4665-b495-856a71b13512")
		)
		(pad "16" thru_hole circle
			(at -4.445 -2 270)
			(size 1 1)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J1-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
			(uuid "1cfbc1dc-6e0a-49ea-9a1b-2d410dc63e39")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 126.5 140)
		(end 120 139.945)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "1b9701a5-059e-4bd8-9355-e2c9518eb486")
	)
	(gr_line
		(start 99.75 145.75)
		(end 109.75 145.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "31c8f62d-0899-4ba0-b80a-00900bc5fcfc")
	)
	(gr_line
		(start 109.75 145.75)
		(end 109.75 139.945)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "3c9abd2b-91a3-4aec-95c1-c8647c6e41ef")
	)
	(gr_line
		(start 100 96)
		(end 126 96)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "4d661e2a-9510-461b-8504-90f994722549")
	)
	(gr_line
		(start 126.5 145.75)
		(end 126.5 140)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6d23da43-7be3-4b55-9174-610d87c2f8e5")
	)
	(gr_line
		(start 105.75 129)
		(end 100 129)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "7bf4650b-dd82-449c-b095-18d174f5f0c9")
	)
	(gr_line
		(start 100 129)
		(end 100 96)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "8268d642-8255-4d5f-8830-3bd339f1ab0f")
	)
	(gr_line
		(start 116 139.945)
		(end 116 145.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "a4569abd-e6c3-4390-932b-f28404385287")
	)
	(gr_line
		(start 126 96)
		(end 126 129)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "b6a3f7d2-4c68-4ecc-b5c3-5fb65b525c78")
	)
	(gr_line
		(start 126 129)
		(end 120 129)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "b6a457b6-5caf-4e28-9260-481968dead15")
	)
	(gr_line
		(start 105.75 139.945)
		(end 99.75 139.945)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "ba734747-73d5-4da0-8cc3-1e7fda79540c")
	)
	(gr_line
		(start 99.75 139.945)
		(end 99.75 145.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "effbd562-166b-4f10-9557-a1a59a0ea99c")
	)
	(gr_line
		(start 116 145.75)
		(end 126.5 145.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "f0d2d060-550b-464f-8330-46f63e96f47f")
	)
	(gr_text "Baby Mobile v5 — github.com/you/baby-mobile"
		(at 116 118 0)
		(layer "B.SilkS")
		(uuid "ab2d28e7-e371-4dce-8027-69df7d50f77c")
		(effects
			(font
				(size 0.4 0.4)
				(thickness 0.08)
			)
		)
	)
	(embedded_fonts no)
)
