(footprint "FLEX-TAIL-FPC16-P0.50"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567801")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "FLEX-TAIL-FPC16"
		(at 0 2.7 0)
		(layer "F.Fab")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567802")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567803")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Flex PCB tail, 16-pin, 0.5mm pitch. Pads 1-16 are 0.3x1.5mm contact fingers on F.Cu matching FPC16-T1T1-2020-A (FPC1). Pad 17=GND tie, 18/19=mechanical anchors. Edge.Cuts define the flex tab on 3 sides (top open, connects to board body). Insert tab into FPC1 with F.Cu face down (bottom-contact type)."
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567804")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_rect
		(start -4.5 -2.7)
		(end 4.5 2.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567810")
	)
	(fp_rect
		(start -4.25 -2.5)
		(end 4.25 2.0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567811")
	)
	(fp_line
		(start -4.5 1.7)
		(end -4.5 -2.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567812")
	)
	(fp_line
		(start 4.5 1.7)
		(end 4.5 -2.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567813")
	)
	(fp_circle
		(center -3.75 -1.8)
		(end -3.65 -1.8)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567814")
	)
	(fp_line
		(start -4.25 2.0)
		(end -4.25 -2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567820")
	)
	(fp_line
		(start -4.25 -2.5)
		(end 4.25 -2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567821")
	)
	(fp_line
		(start 4.25 -2.5)
		(end 4.25 2.0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567822")
	)
	(fp_rect
		(start -4.0 -1.0)
		(end 4.0 1.0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "User.1")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567830")
	)
	(pad "1" smd rect
		(at -3.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567841")
	)
	(pad "2" smd rect
		(at -3.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567842")
	)
	(pad "3" smd rect
		(at -2.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567843")
	)
	(pad "4" smd rect
		(at -2.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567844")
	)
	(pad "5" smd rect
		(at -1.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567845")
	)
	(pad "6" smd rect
		(at -1.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567846")
	)
	(pad "7" smd rect
		(at -0.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567847")
	)
	(pad "8" smd rect
		(at -0.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567848")
	)
	(pad "9" smd rect
		(at 0.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567849")
	)
	(pad "10" smd rect
		(at 0.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567850")
	)
	(pad "11" smd rect
		(at 1.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567851")
	)
	(pad "12" smd rect
		(at 1.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567852")
	)
	(pad "13" smd rect
		(at 2.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567853")
	)
	(pad "14" smd rect
		(at 2.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567854")
	)
	(pad "15" smd rect
		(at 3.25 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567855")
	)
	(pad "16" smd rect
		(at 3.75 0)
		(size 0.3 1.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567856")
	)
	(pad "17" smd rect
		(at 0 1.3)
		(size 1.0 0.5)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567857")
	)
	(pad "18" smd rect
		(at 3.1 1.0)
		(size 0.5 1.0)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567858")
	)
	(pad "19" smd rect
		(at -3.1 1.0)
		(size 0.5 1.0)
		(layers "F.Cu" "F.Mask")
		(uuid "a1b2c3d4-e5f6-7890-abcd-ef1234567859")
	)
	(embedded_fonts no)
)
