(footprint "SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
	(tags "net tie solder jumper bridged")
	(property "Reference" "REF**"
		(at -1.4 0 0)
		(layer "F.SilkS")
		(uuid "7e665f20-2274-46c5-b843-429dec3d10e8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify right)
		)
	)
	(property "Value" "SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(at 1.4 0 0)
		(layer "F.Fab")
		(uuid "47090aa3-9309-4fe1-8b8d-3a99dfbe88f2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "09f04004-e42d-4901-8654-2017adc86ec5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "174271f2-71a3-44be-a2d2-154173802b94")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 1)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(net_tie_pad_groups "1, 2")
	(fp_poly
		(pts
			(xy 0.25 -0.3) (xy -0.25 -0.3) (xy -0.25 0.3) (xy 0.25 0.3)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Cu")
		(uuid "8bc6f947-f49a-4bdd-98e2-b20e557e0211")
	)
	(fp_rect
		(start -0.15 -0.75)
		(end 0.15 0.75)
		(stroke
			(width 0)
			(type default)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "ac23f5fb-85d4-4513-afe3-6cf955101da9")
	)
	(fp_line
		(start -1.4 0.3)
		(end -1.4 -0.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a30b3f4f-61f1-42ad-8536-f5358333dbd7")
	)
	(fp_line
		(start -0.7 -1)
		(end 0.7 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6dd483d2-b998-42e4-90d3-e028559844b4")
	)
	(fp_line
		(start 0.7 1)
		(end -0.7 1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "21f82b70-4b0c-4fdc-981f-c25387bb02c4")
	)
	(fp_line
		(start 1.4 -0.3)
		(end 1.4 0.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dbac6d59-a469-45f1-9d8b-cf4fb0d717ec")
	)
	(fp_arc
		(start -1.4 -0.3)
		(mid -1.194975 -0.794975)
		(end -0.7 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "099f0c6e-f09a-4f36-a7bc-dcb9ad7052ec")
	)
	(fp_arc
		(start -0.7 1)
		(mid -1.194975 0.794975)
		(end -1.4 0.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0facf102-4410-45d1-98c0-376291f19ed2")
	)
	(fp_arc
		(start 0.7 -1)
		(mid 1.194975 -0.794975)
		(end 1.4 -0.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "aac4465c-f519-4e64-bad1-e752edde6ef6")
	)
	(fp_arc
		(start 1.4 0.3)
		(mid 1.194975 0.794975)
		(end 0.7 1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a527c0ce-4964-4cf1-9531-d25d2e6a377d")
	)
	(fp_line
		(start -1.65 -1.25)
		(end -1.65 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b26fc4f4-9fe1-4ea4-8b20-4a6807b0424c")
	)
	(fp_line
		(start -1.65 -1.25)
		(end 1.65 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6acd19c2-033a-4f93-a92b-78f044d3de0c")
	)
	(fp_line
		(start 1.65 1.25)
		(end -1.65 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "665353ca-4e2b-4800-bc88-43129d3b2f09")
	)
	(fp_line
		(start 1.65 1.25)
		(end 1.65 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3f57bb6a-1d91-41bd-84f0-907a6a4f2f94")
	)
	(pad "1" smd custom
		(at -0.65 0)
		(size 1 0.5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 0.25)
				(end 0.5 0.25)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0 -0.25)
				(end 0.5 -0.25)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "9003f6f7-52c6-46a0-bdfb-49f7aa2ac367")
	)
	(pad "2" smd custom
		(at 0.65 0)
		(size 1 0.5)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center 0 0.25)
				(end 0.5 0.25)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0 -0.25)
				(end 0.5 -0.25)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
				)
				(width 0)
				(fill yes)
			)
		)
		(uuid "cb34049a-1987-4949-ab7a-f4fb6fbc034c")
	)
	(embedded_fonts no)
)
