(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 0.1)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(44 "Edge.Cuts" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user "B.Fabrication")
		(49 "F.Fab" user "F.Fabrication")
		(50 "User.1" user)
		(51 "User.2" user)
	)

	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)

	(net 0 "")
	(net 1 "CH01")
	(net 2 "CH02")
	(net 3 "CH03")
	(net 4 "CH04")
	(net 5 "CH05")
	(net 6 "CH06")
	(net 7 "CH07")
	(net 8 "CH08")
	(net 9 "CH09")
	(net 10 "CH10")
	(net 11 "CH11")
	(net 12 "CH12")
	(net 13 "CH13")
	(net 14 "CH14")
	(net 15 "CH15")
	(net 16 "CH16")
	(gr_line
		(start 95.0 87.0)
		(end 105.0 87.0)
		(stroke (width 0.05) (type default))
		(layer "Edge.Cuts")
		(uuid "aa4c43ff-ae4b-4747-9086-e34ace968dc4")
	)
	(gr_line
		(start 105.0 87.0)
		(end 105.0 117.0)
		(stroke (width 0.05) (type default))
		(layer "Edge.Cuts")
		(uuid "abfd57a0-c055-4929-987f-c31eb59d7404")
	)
	(gr_line
		(start 105.0 117.0)
		(end 95.0 117.0)
		(stroke (width 0.05) (type default))
		(layer "Edge.Cuts")
		(uuid "076b95a1-3536-49d9-b06f-0e44b2d4b291")
	)
	(gr_line
		(start 95.0 117.0)
		(end 95.0 87.0)
		(stroke (width 0.05) (type default))
		(layer "Edge.Cuts")
		(uuid "dc0c1ad8-313d-4bdc-a4a3-7b896905e182")
	)
	(gr_line
		(start 95.0 108.0)
		(end 105.0 108.0)
		(stroke (width 0.1) (type default))
		(layer "User.1")
		(uuid "29929131-c9b6-451e-8503-0716752b583b")
	)
	(gr_text "← stiffener above"
		(at 100.0 106.5)
		(layer "User.1")
		(uuid "048ddc95-a144-4711-aec0-d3b16c325d18")
		(effects (font (size 0.6 0.6) (thickness 0.090)))
	)
	(gr_text "bare flex / contact zone ↓"
		(at 100.0 109.5)
		(layer "User.1")
		(uuid "bdc4a9da-815c-4d73-8964-189380ed30a8")
		(effects (font (size 0.6 0.6) (thickness 0.090)))
	)
	(gr_line
		(start 94.85 86.85)
		(end 105.15 86.85)
		(stroke (width 0.05) (type default))
		(layer "F.CrtYd")
		(uuid "246620c7-b6a6-4273-9e30-7e1b1eb97f4e")
	)
	(gr_line
		(start 105.15 86.85)
		(end 105.15 117.15)
		(stroke (width 0.05) (type default))
		(layer "F.CrtYd")
		(uuid "c49f611c-f5f5-4660-9605-5449ccde3023")
	)
	(gr_line
		(start 105.15 117.15)
		(end 94.85 117.15)
		(stroke (width 0.05) (type default))
		(layer "F.CrtYd")
		(uuid "76a330b5-80ba-4339-9aa9-125736d3bd2a")
	)
	(gr_line
		(start 94.85 117.15)
		(end 94.85 86.85)
		(stroke (width 0.05) (type default))
		(layer "F.CrtYd")
		(uuid "930d2bc8-d10f-4a43-b494-79eefa5c340a")
	)
	(gr_line
		(start 95.0 87.0)
		(end 105.0 87.0)
		(stroke (width 0.1) (type default))
		(layer "F.Fab")
		(uuid "f58c7b25-f45b-45ad-82b3-e2114c1e0d3e")
	)
	(gr_line
		(start 105.0 87.0)
		(end 105.0 117.0)
		(stroke (width 0.1) (type default))
		(layer "F.Fab")
		(uuid "5ac255cb-0fdc-4833-8d70-63c8c172e1c4")
	)
	(gr_line
		(start 105.0 117.0)
		(end 95.0 117.0)
		(stroke (width 0.1) (type default))
		(layer "F.Fab")
		(uuid "cd3ee5fa-6607-4476-b96f-f406cdedef9f")
	)
	(gr_line
		(start 95.0 117.0)
		(end 95.0 87.0)
		(stroke (width 0.1) (type default))
		(layer "F.Fab")
		(uuid "a114ff06-7a30-461b-98cb-ae753b5c3d46")
	)
	(gr_text "FLEX-FPC16-CABLE"
		(at 100.0 85.0)
		(layer "F.Fab")
		(uuid "b86760fb-ade8-4d7c-984f-fe490830d30a")
		(effects (font (size 1.0 1.0) (thickness 0.150)))
	)
	(gr_text "Satellite end ↑"
		(at 100.0 88.5)
		(layer "F.SilkS")
		(uuid "0ba9afb3-3002-49fd-83cc-9d99d6630afd")
		(effects (font (size 0.6 0.6) (thickness 0.090)))
	)
	(gr_text "FPC tab end ↓"
		(at 100.0 110.5)
		(layer "F.SilkS")
		(uuid "1cc1e4fe-f2a0-4353-93a5-c68b7de14adc")
		(effects (font (size 0.6 0.6) (thickness 0.090)))
	)
	(gr_text "INSERT B.Cu FACE DOWN"
		(at 100.0 112.0)
		(layer "F.SilkS")
		(uuid "1285b84d-4d08-4484-b1ae-0da4d1a4696d")
		(effects (font (size 0.5 0.5) (thickness 0.075)))
	)
	(gr_circle
		(center 94.855 90.5)
		(end 95.055 90.5)
		(stroke (width 0.1) (type solid))
		(fill yes)
		(layer "F.SilkS")
		(uuid "9aa019ca-683f-47a4-bbd8-f57eff33324c")
	)
	(footprint "FLEX_SAT_PADS"
		(layer "F.Cu")
		(uuid "106de6bb-8647-4a0c-b5e2-78547d4b91d2")
		(at 0 0)
		(property "Reference" "SAT1"
			(at 100.0 88.0 0)
			(layer "F.SilkS")
			(uuid "e2eaaa77-19ac-4be8-a674-dc733db1c42f")
			(effects (font (size 1 1) (thickness 0.15)))
		)
		(property "Value" "A16N-SATELLITE-PADS"
			(at 100.0 89.5 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c25cef03-30ac-4068-bcf0-9ff901f59c96")
			(effects (font (size 1 1) (thickness 0.15)))
		)
		(pad "1" smd rect
			(at 95.555 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "CH01")
			(pinfunction "1")
			(pintype "unspecified")
			(uuid "56e3a545-5ace-45e4-be7e-041144d92b1c")
		)
		(pad "2" smd rect
			(at 96.825 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "CH02")
			(pinfunction "2")
			(pintype "unspecified")
			(uuid "f11b23e7-3810-4658-9349-5e2909759f73")
		)
		(pad "3" smd rect
			(at 98.095 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "CH03")
			(pinfunction "3")
			(pintype "unspecified")
			(uuid "247aedcc-7779-4461-8cf4-3b53572b7ac7")
		)
		(pad "4" smd rect
			(at 99.365 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "CH04")
			(pinfunction "4")
			(pintype "unspecified")
			(uuid "b4a31492-5b17-41c0-90e5-18de5881fce9")
		)
		(pad "5" smd rect
			(at 100.635 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "CH05")
			(pinfunction "5")
			(pintype "unspecified")
			(uuid "909d90a0-545e-4102-b22e-8f6c3a094837")
		)
		(pad "6" smd rect
			(at 101.905 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "CH06")
			(pinfunction "6")
			(pintype "unspecified")
			(uuid "2096f58b-90ee-4683-954a-3a8b05c88a87")
		)
		(pad "7" smd rect
			(at 103.175 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 7 "CH07")
			(pinfunction "7")
			(pintype "unspecified")
			(uuid "f3f71b7a-9b7f-49c2-9f00-be920b0e5ea3")
		)
		(pad "8" smd rect
			(at 104.445 90.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 8 "CH08")
			(pinfunction "8")
			(pintype "unspecified")
			(uuid "605b8b87-2001-41f6-af46-344a6c852e9d")
		)
		(pad "9" smd rect
			(at 104.445 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 9 "CH09")
			(pinfunction "9")
			(pintype "unspecified")
			(uuid "b8adb42a-71c7-4f49-bd7c-f8b6df7374e3")
		)
		(pad "10" smd rect
			(at 103.175 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 10 "CH10")
			(pinfunction "10")
			(pintype "unspecified")
			(uuid "25b9950b-4df9-4c00-85f9-05c7924f15c2")
		)
		(pad "11" smd rect
			(at 101.905 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 11 "CH11")
			(pinfunction "11")
			(pintype "unspecified")
			(uuid "408d0a54-3a46-4717-81d9-ebdf042031eb")
		)
		(pad "12" smd rect
			(at 100.635 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 12 "CH12")
			(pinfunction "12")
			(pintype "unspecified")
			(uuid "dd3c6e65-9ab7-4ba8-9585-c9357ba3929f")
		)
		(pad "13" smd rect
			(at 99.365 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 13 "CH13")
			(pinfunction "13")
			(pintype "unspecified")
			(uuid "6018a000-030d-41d1-957f-592a13907b52")
		)
		(pad "14" smd rect
			(at 98.095 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 14 "CH14")
			(pinfunction "14")
			(pintype "unspecified")
			(uuid "50d99030-8f74-42eb-a04c-6e3351140515")
		)
		(pad "15" smd rect
			(at 96.825 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 15 "CH15")
			(pinfunction "15")
			(pintype "unspecified")
			(uuid "17f5f2a5-3d25-47b2-8242-2bfaf69460a8")
		)
		(pad "16" smd rect
			(at 95.555 94.5)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask")
			(net 16 "CH16")
			(pinfunction "16")
			(pintype "unspecified")
			(uuid "b739e809-f9fc-4f49-a780-6ccbcca9cfe6")
		)
		(fp_line
			(start 94.75500000000001 89.4)
			(end 105.24499999999999 89.4)
			(stroke (width 0.1) (type default))
			(layer "F.SilkS")
			(uuid "8109fd03-0f1c-4b8a-a0bc-941af63f296d")
		)
		(fp_line
			(start 94.75500000000001 95.6)
			(end 105.24499999999999 95.6)
			(stroke (width 0.1) (type default))
			(layer "F.SilkS")
			(uuid "bb4b3eb5-746f-480b-9fa9-32a77d3d9ff0")
		)
		(embedded_fonts no)
	)
	(footprint "FLEX_FPC_FINGERS"
		(layer "F.Cu")
		(uuid "16f35122-5ce1-4f25-a900-73b05c674fc1")
		(at 0 0)
		(property "Reference" "FPC_TAB"
			(at 100.0 115.5 0)
			(layer "F.SilkS")
			(uuid "19e72217-294b-41ea-a009-2446ddef1651")
			(effects (font (size 1 1) (thickness 0.15)))
		)
		(property "Value" "FPC16-0.5mm-BOTTOM-CONTACT"
			(at 100.0 110.5 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bb6cb7f2-35af-461b-9a49-11d32ec55a02")
			(effects (font (size 1 1) (thickness 0.15)))
		)
		(pad "1" smd rect
			(at 96.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 1 "CH01")
			(pinfunction "1")
			(pintype "unspecified")
			(uuid "d7d73ef0-b611-4086-93cf-81bb06e12f49")
		)
		(pad "2" smd rect
			(at 96.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 2 "CH02")
			(pinfunction "2")
			(pintype "unspecified")
			(uuid "56050b14-9154-43c3-8fe3-41ce7b7e9400")
		)
		(pad "3" smd rect
			(at 97.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 3 "CH03")
			(pinfunction "3")
			(pintype "unspecified")
			(uuid "d560edab-c2df-4f9d-b9b3-abd22c0948b9")
		)
		(pad "4" smd rect
			(at 97.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 4 "CH04")
			(pinfunction "4")
			(pintype "unspecified")
			(uuid "5e6d3814-6fc7-4562-accf-c3bfcc6f7a39")
		)
		(pad "5" smd rect
			(at 98.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 5 "CH05")
			(pinfunction "5")
			(pintype "unspecified")
			(uuid "08099728-1b78-40ba-a7ba-47b751afff0a")
		)
		(pad "6" smd rect
			(at 98.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 6 "CH06")
			(pinfunction "6")
			(pintype "unspecified")
			(uuid "bba75bf3-65aa-4dbf-8ea0-e9a13dc01b07")
		)
		(pad "7" smd rect
			(at 99.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 7 "CH07")
			(pinfunction "7")
			(pintype "unspecified")
			(uuid "a00a01e8-9cc7-46e2-8c3a-4f51d61961ae")
		)
		(pad "8" smd rect
			(at 99.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 8 "CH08")
			(pinfunction "8")
			(pintype "unspecified")
			(uuid "952f2814-8286-47e5-a631-b1d30ed26de8")
		)
		(pad "9" smd rect
			(at 100.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 9 "CH09")
			(pinfunction "9")
			(pintype "unspecified")
			(uuid "017c8102-0ea1-4bad-93a2-f03ea3a496e9")
		)
		(pad "10" smd rect
			(at 100.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 10 "CH10")
			(pinfunction "10")
			(pintype "unspecified")
			(uuid "029ecfda-6397-4468-8552-9c6ef7d21783")
		)
		(pad "11" smd rect
			(at 101.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 11 "CH11")
			(pinfunction "11")
			(pintype "unspecified")
			(uuid "12a23b6e-147d-4cb8-9407-87801f645d46")
		)
		(pad "12" smd rect
			(at 101.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 12 "CH12")
			(pinfunction "12")
			(pintype "unspecified")
			(uuid "5672248c-aee0-45f4-a04b-4f1783ad1205")
		)
		(pad "13" smd rect
			(at 102.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 13 "CH13")
			(pinfunction "13")
			(pintype "unspecified")
			(uuid "70eb969c-80bf-4f76-b27f-fd29ff0c84b7")
		)
		(pad "14" smd rect
			(at 102.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 14 "CH14")
			(pinfunction "14")
			(pintype "unspecified")
			(uuid "f3b354ed-f49a-4189-a45a-32d360f9ca5c")
		)
		(pad "15" smd rect
			(at 103.25 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 15 "CH15")
			(pinfunction "15")
			(pintype "unspecified")
			(uuid "a06a53c3-eea5-41d0-8c4c-4fa8996ede07")
		)
		(pad "16" smd rect
			(at 103.75 113.0)
			(size 0.28 3.0)
			(layers "B.Cu")
			(net 16 "CH16")
			(pinfunction "16")
			(pintype "unspecified")
			(uuid "da871259-248d-4f4c-ac7e-6699394172f1")
		)
		(fp_line
			(start 95.0 111.5)
			(end 105.0 111.5)
			(stroke (width 0.05) (type default))
			(layer "F.SilkS")
			(uuid "536ecabe-8eed-4f33-bc87-0032440dd640")
		)
		(fp_line
			(start 95.3 112.0)
			(end 95.3 116.7)
			(stroke (width 0.15) (type default))
			(layer "F.SilkS")
			(uuid "87e48215-77a6-4de8-a3d2-2556ae5d2d0d")
		)
		(fp_line
			(start 104.7 112.0)
			(end 104.7 116.7)
			(stroke (width 0.15) (type default))
			(layer "F.SilkS")
			(uuid "05a4c7ab-cfe3-4dac-a3ab-beb1d7bff07a")
		)
		(fp_line
			(start 95.75 111.0)
			(end 95.75 111.3)
			(stroke (width 0.15) (type default))
			(layer "B.SilkS")
			(uuid "c11501d8-8eea-417c-b808-da15e75318ee")
		)
		(embedded_fonts no)
	)
)
