(footprint "CONN-FPC-SMD_16P-P1.00-O0.50"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "FPC2"
		(at 0 -4 0)
		(layer "F.SilkS")
		(uuid "c4cf29e2-0fc8-49c1-95e1-11a20630aeeb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "FPC-16"
		(at 0 3.5 0)
		(layer "F.Fab")
		(uuid "8c0e3441-8af2-4406-8b1c-a69858e055c6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "cbb681ef-cf2e-4ad1-a1ae-6a47dd935e1e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "17675362-769b-4af3-b736-674e9bfc0aa0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3DModel_Q" "312da58311b441c88ccf7f3f52954456"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "883c8658-1b1e-4224-bf8c-cacf45f511e2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3D_Size" "25 4.4"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "fbc4c6d1-3b94-4077-927f-9a80edc6141e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer Part" "FPC16-T1T1-2020-A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "157c3e12-06ea-4e81-ac02-9879fc32ff1d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer" "SHETIME(高钺达)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "632a2417-c252-4ccb-b5bd-42b9110cfb1a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Supplier Part" "C52740846"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0fa54962-e810-4f0e-9964-25ab1ac7298c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Supplier" "LCSC"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a9d7b505-6206-4098-b62b-757fe25816b0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC Part Name" "翻盖式 下接 P数:16P 间距:0.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3ab2d9cc-80b5-4daa-970d-4a07c87ab013")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_rect
		(start -6 -1.2)
		(end -4.2 1.2)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Cu")
		(uuid "42506433-7fbd-48b9-9018-af7738a016bb")
	)
	(fp_rect
		(start 4.7 -1.2)
		(end 6.5 1.2)
		(stroke
			(width 0)
			(type solid)
		)
		(fill yes)
		(layer "F.Cu")
		(uuid "0842fa47-f564-452e-937a-1d975bcc2281")
	)
	(fp_line
		(start -6.5 -2)
		(end -6.5 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "12b7cbf4-ba14-4211-8d98-f75be29f1ee2")
	)
	(fp_line
		(start -6.5 2.5)
		(end 7 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e3fa00aa-71dd-4b00-b8a3-798b44b4e08a")
	)
	(fp_line
		(start -5.5 -3)
		(end -6.5 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f9b0b97e-10e4-414f-94e0-d4fad34f8111")
	)
	(fp_line
		(start 6 -3)
		(end -5.5 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e07329f1-bcfa-4887-b12c-d5cfc45bad1c")
	)
	(fp_line
		(start 7 -2)
		(end 6 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0007694b-d36c-4821-8786-8da3d8951588")
	)
	(fp_line
		(start 7 2.5)
		(end 7 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3be8df40-ba49-471c-a5ad-bfd796cefa9f")
	)
	(fp_rect
		(start -6.2 -1.4)
		(end -3.8 1.4)
		(stroke
			(width 0.01)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "ef75f980-78ee-4de6-966d-e07fe7186386")
	)
	(fp_rect
		(start 4.3 -1.4)
		(end 6.7 1.4)
		(stroke
			(width 0.01)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "537b1dcc-864a-42ca-9d38-fe257cde524c")
	)
	(fp_circle
		(center -7 3.5)
		(end -6.9 3.5)
		(stroke
			(width 0.254)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "d3fa9cc8-625e-4466-9fd5-81c9178bb698")
	)
	(pad "1" smd rect
		(at -3.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "6fab43c3-9bfd-44a2-ab00-aa839c1ef025")
	)
	(pad "2" smd rect
		(at -3 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "65be5679-8d2c-4baf-92b4-cc786e4dd0c9")
	)
	(pad "3" smd rect
		(at -2.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "0af1b3af-8057-4c02-bf19-d204bfbd0262")
	)
	(pad "4" smd rect
		(at -2 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "db30d023-33b1-4019-9b18-90a65f4d0aa8")
	)
	(pad "5" smd rect
		(at -1.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "9904cbc4-5dc8-4081-9d40-e4a5196bf53f")
	)
	(pad "6" smd rect
		(at -1 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "aa69d731-167d-4dab-b5b6-40169c0b7970")
	)
	(pad "7" smd rect
		(at -0.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "772746e2-270c-4de4-b9a8-dc02a344bd16")
	)
	(pad "8" smd rect
		(at 0 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "eeaf74f0-9a2d-4509-9770-36e0b8871261")
	)
	(pad "9" smd rect
		(at 0.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "e8e1c5d5-2cb9-430f-807a-aa74f798d34d")
	)
	(pad "10" smd rect
		(at 1 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "49f45ba2-ea7c-435d-a0ba-6d60fc537aaa")
	)
	(pad "11" smd rect
		(at 1.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "8eaccd0b-909d-4aea-a3ce-e27c8e14a08c")
	)
	(pad "12" smd rect
		(at 2 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "6e22bcec-9f4a-49cd-8ce7-2fdca0190bf7")
	)
	(pad "13" smd rect
		(at 2.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "0d557cf3-d88e-4331-be9f-e880908c9a83")
	)
	(pad "14" smd rect
		(at 3 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c569763a-9e95-4025-92ea-5a05bb227784")
	)
	(pad "15" smd rect
		(at 3.5 1.25)
		(size 0.6 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "05a3373b-f15d-4fc7-8c29-73316a5dde54")
	)
	(pad "16" smd rect
		(at 4 -1.35)
		(size 0.6 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "f655dd8b-a1c2-4c73-a4f2-81abc3bcf658")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/EASYEDA_MODELS/CONN-SMD_23P-L25.0-W3.0-P1.00-L_TE_2-84982-3.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
