(footprint "TestPoint_Bridge_Pitch2.54mm_Drill1.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "wire loop as test point, pitch 2.54mm, hole diameter 1.0mm, wire diameter 0.8mm")
	(tags "test point wire loop")
	(property "Reference" "JP12"
		(at 7.06 -0.01 0)
		(layer "F.SilkS")
		(uuid "52657ef5-2257-4914-989e-eeb5186debcb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "~"
		(at 1.25 0.87 0)
		(layer "F.Fab")
		(uuid "93846d3d-68c5-4744-9bb3-ef5e1a747edf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ac86c74a-5924-47a7-a2b8-9d5f67781f00")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Solder Jumper, 2-pole, closed/bridged"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0f362018-09c7-4d81-ba6a-8b27ee90b255")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole exclude_from_bom)
	(fp_line
		(start 2.54 0)
		(end 0 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Cu")
		(uuid "dc6cd189-aed9-4aae-ba90-97ce21a94ecb")
	)
	(fp_line
		(start -1.2 -1.2)
		(end -1.2 1.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fcfbb0e1-6d9f-4c2b-8b17-9d34bf2e2eab")
	)
	(fp_line
		(start -1.2 1.2)
		(end 3.7 1.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "97ffbbf2-821b-4b1a-b5d3-17880c9a4066")
	)
	(fp_line
		(start 3.7 -1.2)
		(end -1.2 -1.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d9bfc39b-17de-4a82-9b3b-98a17605467c")
	)
	(fp_line
		(start 3.7 1.2)
		(end 3.7 -1.2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d0879f97-5fbf-4054-957d-0277ff3106b4")
	)
	(fp_line
		(start -1.5 -1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "9e69d66e-66b2-4979-902b-e8c0efff9491")
	)
	(fp_line
		(start -1.5 -1.5)
		(end 4.04 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8cb085a0-63fc-414f-9c7f-6a1abaeabb9b")
	)
	(fp_line
		(start 4.04 1.5)
		(end -1.5 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "24dc771b-fbbd-4de0-bfc6-357c024fdbbc")
	)
	(fp_line
		(start 4.04 1.5)
		(end 4.04 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "0cc5a95c-9b7f-46ae-9521-01557d47a01c")
	)
	(fp_text user "${REFERENCE}"
		(at -2.32 0 0)
		(layer "F.Fab")
		(uuid "6913e19c-125a-4190-a2c5-fb2e6a0319fe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify right)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7997be8f-b557-42c7-b7da-64bb969f5d88")
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fbc49f1f-139e-499e-b0c9-cde15e2230ac")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Bridge_Pitch2.54mm_Drill1.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
