<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="-2.54" x2="0" y2="86.36" width="0.4064" layer="20"/>
<wire x1="0" y1="86.36" x2="78.74" y2="86.36" width="0.4064" layer="20"/>
<wire x1="78.74" y1="86.36" x2="78.74" y2="-2.54" width="0.4064" layer="20"/>
<wire x1="78.74" y1="-2.54" x2="0" y2="-2.54" width="0.4064" layer="20"/>
<text>Open Access Control Interlock v1.1</text>
<text>Will Bradley, zyphon.com/oaci</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>LCD</text>
<text>39919</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="AXIAL-0.3">
</package>
<package name="DUEMILANOVE_VIAS">
</package>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pot">
<packages>
<package name="RS3">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LCD1602">
</package>
<package name="PS12">
</package>
<package name="TO220-NOHOLE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUINO" library="SparkFun" package="DUEMILANOVE_VIAS" value="ARDUINO_SHIELDNO_SILK"/>
<element name="RDR_DATA" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value="SCREW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RDR_PWR" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value="SCREW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY_LED" library="led" package="LED5MM" value="GRN">
<attribute name="NAME"/>
</element>
<element name="WARN_LED" library="led" package="LED5MM" value="RED">
<attribute name="NAME"/>
</element>
<element name="LOGOUT" library="SparkFun" package="TACTILE-PTH" value="btn">
<attribute name="NAME"/>
</element>
<element name="EXTEND" library="SparkFun" package="TACTILE-PTH" value="btn">
<attribute name="NAME"/>
</element>
<element name="SHIFT" library="74xx-eu" package="DIL16" value="74HC595N"/>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="AXIAL-0.3" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONTRAST" library="pot" package="RS3" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="AXIAL-0.3" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RELAY" library="SparkFun" package="SCREWTERMINAL-3.5MM-2" value="SCREW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun" package="STAND-OFF-TIGHT" value=""/>
<element name="U$3" library="SparkFun" package="STAND-OFF-TIGHT" value=""/>
<element name="U$4" library="SparkFun" package="STAND-OFF-TIGHT" value=""/>
<element name="U$5" library="SparkFun" package="STAND-OFF-TIGHT" value=""/>
<element name="LCD" library="adafruit" package="LCD1602" value="HD44780LCD-1602"/>
<element name="SPKR" library="adafruit" package="PS12" value="SPEAKER/PS12"/>
<element name="TIP31C" library="adafruit" package="TO220-NOHOLE" value="TIP30NOHOLE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="AXIAL-0.3" value="220"/>
<element name="R5" library="SparkFun" package="AXIAL-0.3" value="220"/>
<element name="R6" library="SparkFun" package="AXIAL-0.3" value="4.7K"/>
<element name="R7" library="SparkFun" package="AXIAL-0.3" value="4.7K"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="ARDUINO" pad="D2"/>
<contactref element="RDR_DATA" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="ARDUINO" pad="D3"/>
<contactref element="RDR_DATA" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="ARDUINO" pad="5V"/>
<contactref element="SHIFT" pad="16"/>
<contactref element="SHIFT" pad="10"/>
<contactref element="LCD" pad="2"/>
<contactref element="LCD" pad="15"/>
<contactref element="RDR_PWR" pad="1"/>
<contactref element="CONTRAST" pad="A"/>
<contactref element="RELAY" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="SHIFT" pad="14"/>
<contactref element="ARDUINO" pad="D6"/>
</signal>
<signal name="N$6">
<contactref element="SHIFT" pad="12"/>
<contactref element="ARDUINO" pad="D5"/>
</signal>
<signal name="N$7">
<contactref element="SHIFT" pad="11"/>
<contactref element="ARDUINO" pad="D4"/>
</signal>
<signal name="N$9">
<contactref element="ARDUINO" pad="D9"/>
<contactref element="WARN_LED" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="ARDUINO" pad="D8"/>
<contactref element="SPKR" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="SHIFT" pad="8"/>
<contactref element="ARDUINO" pad="GND@0"/>
<contactref element="SHIFT" pad="13"/>
<contactref element="R2" pad="P$1"/>
<contactref element="LCD" pad="1"/>
<contactref element="LCD" pad="5"/>
<contactref element="R1" pad="P$2"/>
<contactref element="EXTEND" pad="2"/>
<contactref element="LOGOUT" pad="2"/>
<contactref element="RDR_PWR" pad="2"/>
<contactref element="CONTRAST" pad="E"/>
<contactref element="SPKR" pad="P$2"/>
<contactref element="TIP31C" pad="3"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="SHIFT" pad="1"/>
<contactref element="LCD" pad="13"/>
</signal>
<signal name="N$4">
<contactref element="SHIFT" pad="2"/>
<contactref element="LCD" pad="12"/>
</signal>
<signal name="N$17">
<contactref element="SHIFT" pad="7"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="SHIFT" pad="15"/>
<contactref element="LCD" pad="14"/>
</signal>
<signal name="N$22">
<contactref element="R3" pad="P$2"/>
<contactref element="WARN_LED" pad="K"/>
</signal>
<signal name="N$8">
<contactref element="ARDUINO" pad="D7"/>
<contactref element="RELAY_LED" pad="A"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="LCD" pad="3"/>
<contactref element="CONTRAST" pad="S"/>
</signal>
<signal name="N$19">
<contactref element="LCD" pad="16"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="SHIFT" pad="3"/>
<contactref element="LCD" pad="11"/>
</signal>
<signal name="N$11">
<contactref element="SHIFT" pad="6"/>
<contactref element="LCD" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="RELAY" pad="2"/>
<contactref element="TIP31C" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="RELAY_LED" pad="K"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$21">
<contactref element="R4" pad="P$2"/>
<contactref element="TIP31C" pad="1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="LOGOUT" pad="4"/>
<contactref element="R6" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="EXTEND" pad="4"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$23">
<contactref element="R6" pad="P$1"/>
<contactref element="ARDUINO" pad="A4"/>
</signal>
<signal name="N$24">
<contactref element="R7" pad="P$1"/>
<contactref element="ARDUINO" pad="A5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
