(footprint "A16N_cast"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "A16N_cast"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "1a5b7791-8f63-45e3-ba51-bdb607dbad8d")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
			(justify mirror)
		)
	)
	(property "Value" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "2a0a9b57-fb2d-4d8d-97df-33d56890bcc6")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
			(justify mirror)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(layer "B.Fab")
		(hide yes)
		(uuid "c1562060-2dc6-40e5-a842-6b0b3718ed71")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(layer "B.Fab")
		(hide yes)
		(uuid "192bfde5-19ee-4adf-bebb-81fd10c34a8a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(fp_line
		(start -5.5 -2)
		(end -5.5 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "d95d3b74-f702-4dcf-b586-73fe612fbf14")
	)
	(fp_line
		(start -5.5 -2)
		(end 5.5 -2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "e0fe8c6c-6f0b-448a-a897-953d8e408995")
	)
	(fp_line
		(start 5.5 -2)
		(end 5.5 -1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "f103481f-9cd7-49fb-9ef8-8cf3f1f18077")
	)
	(fp_line
		(start 5.5 -0.5)
		(end 5.5 0.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9bfdd896-1412-4814-8b18-ff79232de116")
	)
	(fp_line
		(start 5.5 1)
		(end 5.5 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "db0661ce-4ee5-4bf8-b53c-96194948eb78")
	)
	(fp_line
		(start 5.5 2)
		(end -5.5 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6b7c98ed-7f51-4a72-8e5a-c756fc767f63")
	)
	(pad "1" thru_hole circle
		(at -4.445 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c44cc01c-63c6-4a8b-a34a-3f3562f8ea9e")
	)
	(pad "2" thru_hole circle
		(at -3.175 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "20b4f39d-8998-4528-9e8c-b07c1d608b72")
	)
	(pad "3" thru_hole circle
		(at -1.905 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "dcaf6ebc-802a-4edc-b78a-47735327fdff")
	)
	(pad "4" thru_hole circle
		(at -0.635 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6c82a869-868e-4a04-8334-40ed9f56ee40")
	)
	(pad "5" thru_hole circle
		(at 0.635 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f2ea3ef7-f5a6-4f46-8f93-9f71bb5c3d83")
	)
	(pad "6" thru_hole circle
		(at 1.905 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "891692d5-2d1d-48e9-af5e-945a883ed2f0")
	)
	(pad "7" thru_hole circle
		(at 3.175 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ab1ef5fa-f4eb-4baa-8969-fe18b59fcbdd")
	)
	(pad "8" thru_hole circle
		(at 4.445 -2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "ad7db280-4b54-426b-abd1-845d00d42a97")
	)
	(pad "9" thru_hole circle
		(at 4.445 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f35c3503-222a-4918-97b9-3b985d84cab8")
	)
	(pad "10" thru_hole circle
		(at 3.175 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "0620b8ea-907e-4511-a5f6-b80a478020b5")
	)
	(pad "11" thru_hole circle
		(at 1.905 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6b3a7199-3da9-422c-8f9a-8ba41a7f2cee")
	)
	(pad "12" thru_hole circle
		(at 0.635 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f36c9c99-3c1a-4dfa-a0f6-50b842534d06")
	)
	(pad "13" thru_hole circle
		(at -0.635 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "015ee49c-7f11-472e-bed0-149c72b8955e")
	)
	(pad "14" thru_hole circle
		(at -1.905 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b61b8691-2e6c-4bde-914d-11aa3ecf971e")
	)
	(pad "15" thru_hole circle
		(at -3.175 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "264c09ce-3a11-422f-a0ad-fb8732805823")
	)
	(pad "16" thru_hole circle
		(at -4.445 2)
		(size 1 1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "95c7bfdc-ae7b-4377-a98b-d45bd3ab02a2")
	)
	(embedded_fonts no)
)
